(footprint "SW_SPDT_SH_SS-12D07VG4" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Shou Han SPDT SS12D07VG4")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -3.15 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 6e16a0e1-1023-4226-8206-210d4a75c7e1)
  )
  (fp_text value "SW_SPDT_SH_SS-12D07VG4" (at 0 3.4 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 12e825fd-2339-4e58-8a2d-81103f693b13)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.05 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b1a33f99-bb67-4c92-99bd-1ac4293b95b7)
  )
  (fp_line (start -4.5 -2.35) (end 4.5 -2.35)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp a40eb3d1-c5dd-418e-9031-e62defa4a505))
  (fp_line (start -4.5 -1.6) (end -4.5 -2.35)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp b3c66eb9-ba23-4667-8038-9dda000b8203))
  (fp_line (start -4.5 2.35) (end -4.5 1.6)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp f4620975-d028-4388-bf6b-eaba4c84ceea))
  (fp_line (start 4.5 -2.35) (end 4.5 -1.6)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp aa97a4a8-a10f-46d5-bb93-70c27b5348c7))
  (fp_line (start 4.5 1.6) (end 4.5 2.35)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp aa268f46-7076-47b0-991d-247242e8e394))
  (fp_line (start 4.5 2.35) (end -4.5 2.35)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp b0b630b0-ba1e-4c92-be15-c8850cf5735c))
  (fp_line (start -4.35 -2.2) (end 4.35 -2.2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d70caf6a-f7fa-4257-b844-dc8e31bbd6a5))
  (fp_line (start -4.35 -1.6) (end -4.35 -2.2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp b2599d83-ad96-4a13-a559-f82f513996f0))
  (fp_line (start -4.35 1.6) (end -4.35 2.2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 4718000f-a9db-423e-90ac-a3f3b4f7c976))
  (fp_line (start -4.35 2.2) (end 4.35 2.2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 659f872f-b8ce-4756-95a2-cb6db06c489e))
  (fp_line (start 4.35 -2.2) (end 4.35 -1.6)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c86fe7d7-80c5-4cf4-971c-a13869c0cc0d))
  (fp_line (start 4.35 2.2) (end 4.35 1.6)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp b417be3d-ede6-40a0-ae77-e34e3bea6dd0))
  (pad "" thru_hole roundrect (at -4.15 0) (size 1.4 2.2) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp aa42369d-fcff-4584-a804-03310ef94641))
  (pad "" thru_hole roundrect (at 4.15 0) (size 1.4 2.2) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 2e9199f3-088d-466e-8405-1925d3bf81db))
  (pad "1" thru_hole rect (at -2 0) (size 1.2 1.2) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp 38c2caf7-9acd-4795-8d64-bf6dc1f077b7))
  (pad "2" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp 3862c17d-0eae-4ada-a5c5-e2a6e526bc52))
  (pad "3" thru_hole circle (at 2 0) (size 1.2 1.2) (drill 0.6) (layers "*.Cu" "*.Mask") (tstamp accd3dae-d7d7-4d85-a6ae-57ea950e2019))
)
