(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "TCA9416_SOT-23" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TCA9416_SOT-23" (at 5.08 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -10.16 8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "www.ti.com/lit/ds/symlink/tca9416.pdf" (at -7.62 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Bidirectional 1-MHz I2C SMBus Voltage-Level Translator 8kV HBM ESD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Bit Bidirectional 1-MHz, I2C Bus and SMBus Voltage-Level Translator With 8-kV HBM ESD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP*2.95x2.8mm*P0.65mm* VSSOP*2.3x2mm*P0.5mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TCA9416_SOT-23_0_1"
      (rectangle (start -7.62 10.16) (end 7.62 -10.16)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "TCA9416_SOT-23_1_1"
      (pin bidirectional line (at -10.16 0 0) (length 2.54)
        (name "SCL_A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "OE" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 12.7 270) (length 2.54)
        (name "VCCA" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -2.54 0) (length 2.54)
        (name "SDA_A" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -2.54 180) (length 2.54)
        (name "SDA_B" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 12.7 270) (length 2.54)
        (name "VCCB" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 0 180) (length 2.54)
        (name "SCL_B" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TCA9416DDFR" (extends "TCA9416_SOT-23")
    (property "Reference" "U" (at -7.62 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TCA9416D_SOT-23" (at 5.08 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -10.16 8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -7.62 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Bidirectional 1-MHz I2C SMBus Voltage-Level Translator 8kV HBM ESD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Bit Bidirectional 1-MHz, I2C Bus and SMBus Voltage-Level Translator With 8-kV HBM ESD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP*2.95x2.8mm*P0.65mm* VSSOP*2.3x2mm*P0.5mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TCA9416DTMR" (extends "TCA9416_SOT-23")
    (property "Reference" "U" (at -7.62 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TCA9416D_SOT-23" (at 5.08 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8" (at -10.16 8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -7.62 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Bidirectional 1-MHz I2C SMBus Voltage-Level Translator 8kV HBM ESD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Bit Bidirectional 1-MHz, I2C Bus and SMBus Voltage-Level Translator With 8-kV HBM ESD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP*2.95x2.8mm*P0.65mm* VSSOP*2.3x2mm*P0.5mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TCA9416_X2SON" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TCA9416D_SOT-23" (at 5.08 11.43 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (at -10.16 8.89 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "www.ti.com/lit/ds/symlink/tca9416.pdf" (at -7.62 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Bidirectional 1-MHz I2C SMBus Voltage-Level Translator 8kV HBM ESD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2-Bit Bidirectional 1-MHz, I2C Bus and SMBus Voltage-Level Translator With 8-kV HBM ESD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SSOP*2.95x2.8mm*P0.65mm* VSSOP*2.3x2mm*P0.5mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TCA9416_X2SON_0_1"
      (rectangle (start -7.62 10.16) (end 7.62 -10.16)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "TCA9416_X2SON_1_1"
      (pin bidirectional line (at -10.16 0 0) (length 2.54)
        (name "SCL_A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 12.7 270) (length 2.54)
        (name "VCCA" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -2.54 0) (length 2.54)
        (name "SDA_A" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.7 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -2.54 180) (length 2.54)
        (name "SDA_B" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 12.7 270) (length 2.54)
        (name "VCCB" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 0 180) (length 2.54)
        (name "SCL_B" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "OE" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
