(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "Adafruit_HUZZAH32_ESP32_Breakout" (in_bom yes) (on_board yes)
    (property "Reference" "A" (at -12.7 29.21 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "Adafruit_HUZZAH32_ESP32_Breakout" (at 2.54 -31.75 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Asym_MCU_Module:Adafruit_HUZZAH32" (at 2.54 -34.29 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://www.adafruit.com/product/4172" (at 0 -30.48 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Adafruit feather microcontroller module USB" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Microcontroller module with ESP32 MCU" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Adafruit*Feather*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Adafruit_HUZZAH32_ESP32_Breakout_0_1"
      (rectangle (start -12.7 27.94) (end 12.7 -30.48)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "Adafruit_HUZZAH32_ESP32_Breakout_1_1"
      (pin input line (at 15.24 20.32 180) (length 2.54)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
        (name "T7/IO27" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
        (name "T6/IO14" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
        (name "T5/IO12" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
        (name "T4/IO13" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 30.48 270) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -33.02 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 30.48 270) (length 2.54)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
        (name "T3/IO15" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
        (name "T2/IO2" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
        (name "T1/IO0" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 15.24 180) (length 2.54)
        (name "I36" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -20.32 180) (length 2.54)
        (name "T0/IO4" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 5.08 0) (length 2.54)
        (name "IO16" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 2.54 0) (length 2.54)
        (name "IO17" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 0 0) (length 2.54)
        (name "IO5" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 2.54)
        (name "IO18" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -5.08 0) (length 2.54)
        (name "IO19" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -12.7 0) (length 2.54)
        (name "SDA/IO21" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 20.32 0) (length 2.54)
        (name "RX/IO9" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 17.78 0) (length 2.54)
        (name "TX/IO10" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -15.24 0) (length 2.54)
        (name "SCL/IO22" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 12.7 180) (length 2.54)
        (name "I39" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -7.62 0) (length 2.54)
        (name "IO23" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 10.16 180) (length 2.54)
        (name "I34/A2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 15.24 7.62 180) (length 2.54)
        (name "I35/A13" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
        (name "T9/IO32" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 2.54)
        (name "T8/IO33" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 12.7 0) (length 2.54)
        (name "DAC1/IO25" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 10.16 0) (length 2.54)
        (name "DAC2/IO26" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
