{
  "board": {
    "3dviewports": [],
    "design_settings": {
      "defaults": {
        "apply_defaults_to_fp_fields": false,
        "apply_defaults_to_fp_shapes": false,
        "apply_defaults_to_fp_text": false,
        "board_outline_line_width": 0.05,
        "copper_line_width": 0.2,
        "copper_text_italic": false,
        "copper_text_size_h": 1.5,
        "copper_text_size_v": 1.5,
        "copper_text_thickness": 0.3,
        "copper_text_upright": false,
        "courtyard_line_width": 0.05,
        "dimension_precision": 4,
        "dimension_units": 3,
        "dimensions": {
          "arrow_length": 1270000,
          "extension_offset": 500000,
          "keep_text_aligned": true,
          "suppress_zeroes": true,
          "text_position": 0,
          "units_format": 0
        },
        "fab_line_width": 0.1,
        "fab_text_italic": false,
        "fab_text_size_h": 1.0,
        "fab_text_size_v": 1.0,
        "fab_text_thickness": 0.15,
        "fab_text_upright": false,
        "other_line_width": 0.1,
        "other_text_italic": false,
        "other_text_size_h": 1.0,
        "other_text_size_v": 1.0,
        "other_text_thickness": 0.15,
        "other_text_upright": false,
        "pads": {
          "drill": 0.0,
          "height": 0.245,
          "width": 0.245
        },
        "silk_line_width": 0.1,
        "silk_text_italic": false,
        "silk_text_size_h": 1.0,
        "silk_text_size_v": 1.0,
        "silk_text_thickness": 0.1,
        "silk_text_upright": false,
        "zones": {
          "min_clearance": 0.5
        }
      },
      "diff_pair_dimensions": [
        {
          "gap": 0.0,
          "via_gap": 0.0,
          "width": 0.0
        }
      ],
      "drc_exclusions": [],
      "meta": {
        "version": 2
      },
      "rule_severities": {
        "annular_width": "error",
        "clearance": "error",
        "connection_width": "warning",
        "copper_edge_clearance": "error",
        "copper_sliver": "warning",
        "courtyards_overlap": "error",
        "creepage": "error",
        "diff_pair_gap_out_of_range": "error",
        "diff_pair_uncoupled_length_too_long": "error",
        "drill_out_of_range": "error",
        "duplicate_footprints": "warning",
        "extra_footprint": "warning",
        "footprint": "error",
        "footprint_filters_mismatch": "ignore",
        "footprint_symbol_mismatch": "warning",
        "footprint_type_mismatch": "ignore",
        "hole_clearance": "error",
        "hole_to_hole": "warning",
        "holes_co_located": "warning",
        "invalid_outline": "error",
        "isolated_copper": "warning",
        "item_on_disabled_layer": "error",
        "items_not_allowed": "error",
        "length_out_of_range": "error",
        "lib_footprint_issues": "warning",
        "lib_footprint_mismatch": "warning",
        "malformed_courtyard": "error",
        "microvia_drill_out_of_range": "error",
        "mirrored_text_on_front_layer": "warning",
        "missing_courtyard": "ignore",
        "missing_footprint": "warning",
        "net_conflict": "warning",
        "nonmirrored_text_on_back_layer": "warning",
        "npth_inside_courtyard": "ignore",
        "padstack": "warning",
        "pth_inside_courtyard": "ignore",
        "shorting_items": "error",
        "silk_edge_clearance": "warning",
        "silk_over_copper": "warning",
        "silk_overlap": "warning",
        "skew_out_of_range": "error",
        "solder_mask_bridge": "error",
        "starved_thermal": "error",
        "text_height": "warning",
        "text_on_edge_cuts": "error",
        "text_thickness": "warning",
        "through_hole_pad_without_hole": "error",
        "too_many_vias": "error",
        "track_angle": "error",
        "track_dangling": "warning",
        "track_segment_length": "error",
        "track_width": "error",
        "tracks_crossing": "error",
        "unconnected_items": "error",
        "unresolved_variable": "error",
        "via_dangling": "warning",
        "zones_intersect": "error"
      },
      "rules": {
        "max_error": 0.005,
        "min_clearance": 0.0,
        "min_connection": 0.0,
        "min_copper_edge_clearance": 0.5,
        "min_groove_width": 0.0,
        "min_hole_clearance": 0.25,
        "min_hole_to_hole": 0.25,
        "min_microvia_diameter": 0.2,
        "min_microvia_drill": 0.1,
        "min_resolved_spokes": 2,
        "min_silk_clearance": 0.0,
        "min_text_height": 0.8,
        "min_text_thickness": 0.08,
        "min_through_hole_diameter": 0.3,
        "min_track_width": 0.0,
        "min_via_annular_width": 0.1,
        "min_via_diameter": 0.5,
        "solder_mask_to_copper_clearance": 0.0,
        "use_height_for_length_calcs": true
      },
      "teardrop_options": [
        {
          "td_onpthpad": true,
          "td_onroundshapesonly": false,
          "td_onsmdpad": true,
          "td_ontrackend": false,
          "td_onvia": true
        }
      ],
      "teardrop_parameters": [
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_round_shape",
          "td_width_to_size_filter_ratio": 0.9
        },
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_rect_shape",
          "td_width_to_size_filter_ratio": 0.9
        },
        {
          "td_allow_use_two_tracks": true,
          "td_curve_segcount": 0,
          "td_height_ratio": 1.0,
          "td_length_ratio": 0.5,
          "td_maxheight": 2.0,
          "td_maxlen": 1.0,
          "td_on_pad_in_zone": false,
          "td_target_name": "td_track_end",
          "td_width_to_size_filter_ratio": 0.9
        }
      ],
      "track_widths": [
        0.0,
        0.09
      ],
      "tuning_pattern_settings": {
        "diff_pair_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 1.0
        },
        "diff_pair_skew_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 0.6
        },
        "single_track_defaults": {
          "corner_radius_percentage": 80,
          "corner_style": 1,
          "max_amplitude": 1.0,
          "min_amplitude": 0.2,
          "single_sided": false,
          "spacing": 0.6
        }
      },
      "via_dimensions": [
        {
          "diameter": 0.0,
          "drill": 0.0
        }
      ],
      "zones_allow_external_fillets": false
    },
    "ipc2581": {
      "dist": "",
      "distpn": "",
      "internal_id": "",
      "mfg": "",
      "mpn": ""
    },
    "layer_pairs": [],
    "layer_presets": [],
    "viewports": []
  },
  "boards": [],
  "cvpcb": {
    "equivalence_files": []
  },
  "libraries": {
    "pinned_footprint_libs": [],
    "pinned_symbol_libs": []
  },
  "meta": {
    "filename": "Test_4-panel_801.kicad_pro",
    "version": 3
  },
  "net_settings": {
    "classes": [
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Default",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 2147483647,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Board_0-Default",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 2147483647,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      },
      {
        "bus_width": 12,
        "clearance": 0.2,
        "diff_pair_gap": 0.25,
        "diff_pair_via_gap": 0.25,
        "diff_pair_width": 0.2,
        "line_style": 0,
        "microvia_diameter": 0.3,
        "microvia_drill": 0.1,
        "name": "Board_1-Default",
        "pcb_color": "rgba(0, 0, 0, 0.000)",
        "priority": 2147483647,
        "schematic_color": "rgba(0, 0, 0, 0.000)",
        "track_width": 0.2,
        "via_diameter": 0.6,
        "via_drill": 0.3,
        "wire_width": 6
      }
    ],
    "meta": {
      "version": 4
    },
    "net_colors": null,
    "netclass_assignments": null,
    "netclass_patterns": [
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.15-Pad8)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/Load Cell Amp/SIG+"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.31-Pad12)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.24-Pad48)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/Power and Interface/SWDIO"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/BLE Controller/~{PAIR_SW}"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-VDD"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.21-Pad43)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/BLE Controller/~{LOAD_CELL_EN}"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U5-PROG)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.01-Pad18)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(Q2-S)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.00-Pad17)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.26-Pad19)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/BLE Controller/SCL"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.00-Pad47)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-GND"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.03-Pad60)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/BLE Controller/~{BATT_INT}"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U4-BIN)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.05-Pad59)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.17-Pad41)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.02-Pad11)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.10-Pad3)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U1B--)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.16-Pad38)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.15-Pad39)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-D+-Pad35)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(J3-SWO{slash}TDO-Pad6)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.06-Pad22)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(R5-Pad1)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U3-SWDIO)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U3-DCCH)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/BLE Controller/~{PAIR_LED}"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-VBUS-Pad32)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.14-Pad7)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-D--Pad34)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.09-Pad26)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/Load Cell Amp/SIG-"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(J3-NC{slash}TDI-Pad8)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U1A--)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/Power and Interface/SWDCLK"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-+3.3V"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(J1-Pin_1)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-VBUS"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/Power and Interface/CHARGE_LED_IO"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.13-Pad6)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U1A-+)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.07-Pad58)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.07-Pad23)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.28-Pad13)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U2A--)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/Load Cell Amp/EXC+"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.30-Pad14)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/BLE Controller/SDA"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.29-Pad10)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.19-Pad42)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.08-Pad24)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.08-Pad25)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.23-Pad45)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.03-Pad9)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U2B--)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(Q3-S)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/Power and Interface/STAT"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/Power and Interface/PAIR_LED_IO"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.10-Pad54)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.13-Pad37)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.25-Pad49)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/BLE Controller/LOAD_CELL"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.22-Pad46)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.12-Pad5)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U3-SWDCLK)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.04-Pad56)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.05-Pad21)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.01-Pad61)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-Net-(U4-VDD)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(J3-KEY-Pad7)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P0.09-Pad52)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-unconnected-(U3-P1.06-Pad57)"
      },
      {
        "netclass": "Board_0-Default",
        "pattern": "Board_0-/Project Architecture/Power and Interface/~{RESET}"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/Load Cell Amp/SIG-"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(J3-NC{slash}TDI-Pad8)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.00-Pad17)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U1B--)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/Power and Interface/STAT"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.30-Pad14)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U4-VDD)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.19-Pad42)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(Q2-S)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.22-Pad46)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(J3-SWO{slash}TDO-Pad6)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/BLE Controller/~{PAIR_LED}"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.00-Pad47)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(J1-Pin_1)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.15-Pad8)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.08-Pad25)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U1A-+)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.13-Pad6)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-+3.3V"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/BLE Controller/SDA"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.07-Pad23)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-D--Pad34)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.07-Pad58)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/BLE Controller/~{LOAD_CELL_EN}"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.13-Pad37)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.10-Pad3)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.21-Pad43)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/Power and Interface/~{RESET}"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/BLE Controller/SCL"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.25-Pad49)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(Q3-S)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/Power and Interface/SWDCLK"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/BLE Controller/~{PAIR_SW}"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.16-Pad38)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-VBUS"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.23-Pad45)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U3-SWDCLK)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.28-Pad13)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/Power and Interface/PAIR_LED_IO"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.01-Pad18)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.24-Pad48)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.03-Pad9)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.02-Pad11)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-GND"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.14-Pad7)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.09-Pad52)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.29-Pad10)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.06-Pad57)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(R5-Pad1)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.26-Pad19)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.01-Pad61)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.10-Pad54)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U3-SWDIO)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/Power and Interface/SWDIO"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/BLE Controller/LOAD_CELL"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.08-Pad24)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.12-Pad5)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/Power and Interface/CHARGE_LED_IO"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U4-BIN)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.09-Pad26)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U1A--)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/Load Cell Amp/SIG+"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/BLE Controller/~{BATT_INT}"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U3-DCCH)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.04-Pad56)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.15-Pad39)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.17-Pad41)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-/Project Architecture/Load Cell Amp/EXC+"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U2A--)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.05-Pad21)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U5-PROG)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-D+-Pad35)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-VBUS-Pad32)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-Net-(U2B--)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.06-Pad22)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P0.31-Pad12)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-VDD"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.03-Pad60)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(U3-P1.05-Pad59)"
      },
      {
        "netclass": "Board_1-Default",
        "pattern": "Board_1-unconnected-(J3-KEY-Pad7)"
      }
    ]
  },
  "pcbnew": {
    "last_paths": {
      "gencad": "",
      "idf": "",
      "netlist": "",
      "plot": "",
      "pos_files": "",
      "specctra_dsn": "",
      "step": "",
      "svg": "",
      "vrml": ""
    },
    "page_layout_descr_file": ""
  },
  "schematic": {
    "legacy_lib_dir": "",
    "legacy_lib_list": []
  },
  "sheets": [],
  "text_variables": {
    "ASSEMBLY_NAME": "Assembly Name",
    "ASSEMBLY_NOTES": "",
    "ASSEMBLY_NUMBER": "A99-9000",
    "ASSEMBLY_SCALE": "1",
    "COMPANY": "Asymworks, LLC",
    "DESIGNER": "JPK",
    "DWG_NUMBER_PCB": "P99-9000",
    "DWG_NUMBER_SCH": "S99-9000",
    "DWG_TITLE_ASSY": "PCB Assembly, Assembly Name",
    "DWG_TITLE_PCB": "PCB, Assembly Name",
    "DWG_TITLE_SCH": "Schematic, Assembly Name",
    "FABRICATION_NOTES": "FABRICATION NOTES (UNLESS OTHERWISE SPECIFIED)\n\n1)\tFABRICATE PER IPC-6012A CLASS 2.\n\n2)\tOUTLINE DEFINED IN SEPARATE GERBER FILE WITH\n\t\"Edge_Cuts.GBR\" SUFFIX.\n\n3)\tSEE SEPARATE DRILL FILES WITH \".DRL\" SUFFIX \n\tFOR HOLE LOCATIONS.\n\n\tSELECTED HOLE LOCATIONS SHOWN ON THIS DRAWING \n\tFOR REFERENCE ONLY.\n\n4)\tSURFACE FINISH: HAL SNPB\n\n5)\tSOLDERMASK ON BOTH SIDES OF THE BOARD SHALL \n\tBE LPI, COLOR GREEN.\n\n6)\tSILK SCREEN LEGEND TO BE APPLIED PER LAYER \n\tSTACKUP USING WHITE NON-CONDUCTIVE EPOXY INK.\n\n7)\tALL VIAS ARE TENTED ON BOTH SIDES UNLESS \n\tSOLDERMASK OPENED IN GERBER.\n\n8)\tRESERVED\n\n9)\tPCB MATERIAL REQUIREMENTS:\n\n\tA.\tFLAMMABILITY RATING MUST MEET OR EXCEED \n\t\tUL94V-0 REQUIREMENTS.\n\tB.\tTg 135 C OR EQUIVALENT.\n\n10)\tDESIGN GEOMETRY MINIMUM FEATURE SIZES:\n\n\tBOARD SIZE\t\t\t\t46.000 \u00d7 27.500 mm\n\tBOARD THICKNESS\t\t1.647 mm\n\tTRACE WIDTH\t\t\t0.100 mm\n\tTRACE TO TRACE\t\t0.200 mm\n\tMIN. HOLE (PTH)\t\t\t0.300 mm\n\tMIN. HOLE (NPTH)\t\t2.200 mm\n\tANNULAR RING\t\t\t0.150 mm\n\tCOPPER TO HOLE\t\t0.250 mm\n\tCOPPER TO EDGE\t\t0.500 mm\n\tHOLE TO HOLE\t\t\t0.250 mm",
    "GIT_HASH": "e4c0a21",
    "GIT_HASH_PCB": "63caa9f",
    "GIT_HASH_SCH": "3dec5ef",
    "GIT_URL": "/jkrauss/Test_4",
    "PROJECT_CODE": "P99",
    "RELEASE_DATE": "2026-03-06",
    "RELEASE_STATE": "WORKING",
    "REVISION": "NO_TAG+ (Unreleased)",
    "SCALE": "2:1",
    "SCHEMATIC_NOTES": "Unless otherwise specified, Resistor Values are in ohms, Capacitor Values are in \u00b5F, and Inductor Values are in \u00b5H.\n\nIn theory this should immediately show up since it's pre-processed before set_text_variables gets called. Now it should even import since the filename is fixed!",
    "SHEET_NAME_01": "Cover Page",
    "SHEET_NAME_02": "Block Diagram",
    "SHEET_NAME_03": "Project Architecture",
    "SHEET_NAME_04": "Load Cell Amp",
    "SHEET_NAME_05": "BLE Controller",
    "SHEET_NAME_06": "Power and Interface",
    "SHEET_NAME_07": "Parts List",
    "SHEET_NAME_08": "......................................",
    "SHEET_NAME_09": "......................................",
    "SHEET_NAME_10": "......................................",
    "SHEET_NAME_11": "......................................",
    "SHEET_NAME_12": "......................................",
    "SHEET_NAME_13": "......................................",
    "SHEET_NAME_14": "......................................",
    "SHEET_NAME_15": "......................................",
    "SHEET_NAME_16": "......................................",
    "SHEET_NAME_17": "......................................",
    "SHEET_NAME_18": "......................................",
    "SHEET_NAME_19": "......................................",
    "SHEET_NAME_20": "......................................",
    "STATE": "TEMPLATE",
    "VARIANT": ""
  }
}