(export (version "E")
  (design
    (source "/workspace/jkrauss/Test_5/Test_5.kicad_sch")
    (date "Date")
    (tool "Eeschema 9.0.7+1")
    (textvar (name "ASSEMBLY_NAME") "Assembly Name")
    (textvar (name "ASSEMBLY_NOTES") "ASSEMBLY NOTES (UNLESS OTHERWISE SPECIFIED)\n\n1)	DO NOT POPULATE COMPONENTS ARE MARKED WITH A RED CROSS\n\n2)	DO NOT POPULATE COMPONENTS ARE NOT PRESENT IN THE BOM\n\n3)	IF CONFLICTING INFORMATION IS FOUND BETWEEN THE ASSEMBLY\n	FILE AND BOM, BOM SHOULD BE USED AS THE MAIN SOURCE.\n\n4)	DOT IDENTIFIES PIN #1 LOCATION AND DEVICE ORIENTATION\n	WHEN VIEWED FROM THE TOP.")
    (textvar (name "ASSEMBLY_NUMBER") "A99-9000")
    (textvar (name "ASSEMBLY_SCALE") "1")
    (textvar (name "COMPANY") "Asymworks, LLC")
    (textvar (name "DESIGNER") "JPK")
    (textvar (name "DWG_NUMBER_PCB") "P99-9000")
    (textvar (name "DWG_NUMBER_SCH") "S99-9000")
    (textvar (name "DWG_TITLE_ASSY") "PCB Assembly, Assembly Name")
    (textvar (name "DWG_TITLE_PCB") "PCB, Assembly Name")
    (textvar (name "DWG_TITLE_SCH") "Schematic, Assembly Name")
    (textvar (name "FABRICATION_NOTES") "FABRICATION NOTES (UNLESS OTHERWISE SPECIFIED)\n\n1)	FABRICATE PER IPC-6012A CLASS 2.\n\n2)	OUTLINE DEFINED IN SEPARATE GERBER FILE WITH\n	\"Edge_Cuts.GBR\" SUFFIX.\n\n3)	SEE SEPARATE DRILL FILES WITH \".DRL\" SUFFIX \n	FOR HOLE LOCATIONS.\n\n	SELECTED HOLE LOCATIONS SHOWN ON THIS DRAWING \n	FOR REFERENCE ONLY.\n\n4)	SURFACE FINISH: HAL SNPB\n\n5)	SOLDERMASK ON BOTH SIDES OF THE BOARD SHALL \n	BE LPI, COLOR GREEN.\n\n6)	SILK SCREEN LEGEND TO BE APPLIED PER LAYER \n	STACKUP USING WHITE NON-CONDUCTIVE EPOXY INK.\n\n7)	ALL VIAS ARE TENTED ON BOTH SIDES UNLESS \n	SOLDERMASK OPENED IN GERBER.\n\n8)	RESERVED\n\n9)	PCB MATERIAL REQUIREMENTS:\n\n	A.	FLAMMABILITY RATING MUST MEET OR EXCEED \n		UL94V-0 REQUIREMENTS.\n	B.	Tg 135 C OR EQUIVALENT.\n\n10)	DESIGN GEOMETRY MINIMUM FEATURE SIZES:\n\n	BOARD SIZE				46.000 × 27.500 mm\n	BOARD THICKNESS		1.647 mm\n	TRACE WIDTH			0.100 mm\n	TRACE TO TRACE		0.200 mm\n	MIN. HOLE (PTH)			0.300 mm\n	MIN. HOLE (NPTH)		2.200 mm\n	ANNULAR RING			0.150 mm\n	COPPER TO HOLE		0.250 mm\n	COPPER TO EDGE		0.500 mm\n	HOLE TO HOLE			0.250 mm\n\n11)	ALL DIMENSIONS ARE IN MILLIMETERS UNLESS OTHERWISE\n	SPECIFIED.\n\n12)	FOR REFERENCE ONLY THE STACKUP CORRESPONDS TO JLCPCB\n	STACKUP JLC04161H-7628.\n	FOR REFERENCE ONLY. IMPEDANCE IS THE CONTROLLING PARAMETER\n	OVER LAYER STACKUP. GERBER DATA MAY NOT BE ALTERED EXCEPT\n	FOR STANDARD FABRICATION ALLOWANCES.\n\n	THE SUPPLIED ARTWORK MAY OR MAY NOT CONTAIN THE SPECIFIED\n	TRACE GEOMETRIES ON EVERY LAYERS SPECIFIED.")
    (textvar (name "GIT_HASH") "17ccbe1")
    (textvar (name "GIT_HASH_PCB") "17ccbe1")
    (textvar (name "GIT_HASH_SCH") "5caa450")
    (textvar (name "GIT_URL") "/jkrauss/Test_4")
    (textvar (name "PROJECT_CODE") "P99")
    (textvar (name "RELEASE_DATE") "2026-03-09")
    (textvar (name "RELEASE_STATE") "WORKING")
    (textvar (name "REVISION") "NO_TAG+ (Unreleased)")
    (textvar (name "SCALE") "2:1")
    (textvar (name "SCHEMATIC_NOTES") "Unless otherwise specified, components Values are in ohms, µF, and µH.")
    (textvar (name "SHEET_NAME_01") "Cover Page")
    (textvar (name "SHEET_NAME_02") "Block Diagram")
    (textvar (name "SHEET_NAME_03") "Project Architecture")
    (textvar (name "SHEET_NAME_04") "Load Cell Amp")
    (textvar (name "SHEET_NAME_05") "BLE Controller")
    (textvar (name "SHEET_NAME_06") "Power and Interface")
    (textvar (name "SHEET_NAME_07") "Parts List")
    (textvar (name "SHEET_NAME_08") "......................................")
    (textvar (name "SHEET_NAME_09") "......................................")
    (textvar (name "SHEET_NAME_10") "......................................")
    (textvar (name "SHEET_NAME_11") "......................................")
    (textvar (name "SHEET_NAME_12") "......................................")
    (textvar (name "SHEET_NAME_13") "......................................")
    (textvar (name "SHEET_NAME_14") "......................................")
    (textvar (name "SHEET_NAME_15") "......................................")
    (textvar (name "SHEET_NAME_16") "......................................")
    (textvar (name "SHEET_NAME_17") "......................................")
    (textvar (name "SHEET_NAME_18") "......................................")
    (textvar (name "SHEET_NAME_19") "......................................")
    (textvar (name "SHEET_NAME_20") "......................................")
    (textvar (name "STATE") "TEMPLATE")
    (textvar (name "VARIANT"))
    (sheet (number "1") (name "/") (tstamps "/")
      (title_block
        (title "Title Page")
        (company "Asymworks, LLC")
        (rev "NO_TAG+ (Unreleased)")
        (date "Date")
        (source "Test_5.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "2") (name "/Block Diagram/") (tstamps "/28ad8293-baaf-4ee1-8056-ad34096542a0/")
      (title_block
        (title "Block Diagram")
        (company "Asymworks, LLC")
        (rev "NO_TAG+ (Unreleased)")
        (date)
        (source "Block_Diagram.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "3") (name "/Project Architecture/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/")
      (title_block
        (title "Project Architecture")
        (company "Asymworks, LLC")
        (rev "NO_TAG+ (Unreleased)")
        (date)
        (source "Architecture.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "4") (name "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/")
      (title_block
        (title "Load Cell Amp")
        (company "Asymworks, LLC")
        (rev "NO_TAG+ (Unreleased)")
        (date)
        (source "Load_Cell_Amp.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "5") (name "/Project Architecture/BLE Controller/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/9da43fd7-7a0a-403c-bf2c-ba67cd8fa669/")
      (title_block
        (title "Circuit 2")
        (company "Asymworks, LLC")
        (rev "NO_TAG+ (Unreleased)")
        (date)
        (source "BLE_Controller.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "6") (name "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/")
      (title_block
        (title "Battery Interface")
        (company "Asymworks, LLC")
        (rev "NO_TAG+ (Unreleased)")
        (date)
        (source "Power_Interface.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "7") (name "/Parts List/") (tstamps "/20edd200-9383-4d87-bd58-f882adb4f112/")
      (title_block
        (title "Parts List")
        (company "Asymworks, LLC")
        (rev "NO_TAG+ (Unreleased)")
        (date)
        (source "Parts_List.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value "")))))
  (components
    (comp (ref "C1")
      (value "100n")
      (footprint "Capacitor_SMD:C_0603_1608Metric")
      (datasheet "https://yageogroup.com/download/specsheet/CC0603KRX7R9BB104")
      (description "capacitor, small US symbol")
      (fields
        (field (name "Manufacturer") "YAGEO")
        (field (name "Manufacturer PN") "CC0603KRX7R9BB104")
        (field (name "LCSC") "C14663")
        (field (name "Footprint") "Capacitor_SMD:C_0603_1608Metric")
        (field (name "Datasheet") "https://yageogroup.com/download/specsheet/CC0603KRX7R9BB104")
        (field (name "Description") "capacitor, small US symbol"))
      (libsource (lib "Device") (part "C_Small_US") (description "capacitor, small US symbol"))
      (property (name "Manufacturer") (value "YAGEO"))
      (property (name "Manufacturer PN") (value "CC0603KRX7R9BB104"))
      (property (name "LCSC") (value "C14663"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "62133f73-88eb-4da2-9491-8bf214c6001b"))
    (comp (ref "C2")
      (value "100n")
      (footprint "Capacitor_SMD:C_0603_1608Metric")
      (datasheet "https://yageogroup.com/download/specsheet/CC0603KRX7R9BB104")
      (description "capacitor, small US symbol")
      (fields
        (field (name "Manufacturer") "YAGEO")
        (field (name "Manufacturer PN") "CC0603KRX7R9BB104")
        (field (name "LCSC") "C14663")
        (field (name "Footprint") "Capacitor_SMD:C_0603_1608Metric")
        (field (name "Datasheet") "https://yageogroup.com/download/specsheet/CC0603KRX7R9BB104")
        (field (name "Description") "capacitor, small US symbol"))
      (libsource (lib "Device") (part "C_Small_US") (description "capacitor, small US symbol"))
      (property (name "Manufacturer") (value "YAGEO"))
      (property (name "Manufacturer PN") (value "CC0603KRX7R9BB104"))
      (property (name "LCSC") (value "C14663"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "9db50cc5-6ad0-42fa-8e86-82db202d88fb"))
    (comp (ref "Q1")
      (value "Si2301CDS")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "https://www.vishay.com/doc/?68741")
      (description "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23")
      (fields
        (field (name "Manufacturer") "Vishay")
        (field (name "Manufacturer PN") "Si2301CDS-T1-GE3")
        (field (name "LCSC") "C10487")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "https://www.vishay.com/doc/?68741")
        (field (name "Description") "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23"))
      (libsource (lib "Asym_Transistor_FET") (part "Si2301CDS") (description "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23"))
      (property (name "Manufacturer") (value "Vishay"))
      (property (name "Manufacturer PN") (value "Si2301CDS-T1-GE3"))
      (property (name "LCSC") (value "C10487"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "P-Channel MOSFET"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "33b05de2-8cc7-48b9-b094-7ba5e6a40724"))
    (comp (ref "R1")
      (value "10k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF1002T5E")
        (field (name "LCSC") "C25804")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF1002T5E"))
      (property (name "LCSC") (value "C25804"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "a9fa5cb8-cb9a-4485-a2e3-7ece0390081e"))
    (comp (ref "R2")
      (value "51k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF5102T5E")
        (field (name "LCSC") "C23196")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF5102T5E"))
      (property (name "LCSC") (value "C23196"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "ef51c143-7984-47c3-bcc3-5b8731aa5a16"))
    (comp (ref "R3")
      (value "51k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF5102T5E")
        (field (name "LCSC") "C23196")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF5102T5E"))
      (property (name "LCSC") (value "C23196"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "0c986be8-745b-4edb-96c4-f8ea61e9db02"))
    (comp (ref "R4")
      (value "220k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF2203T5E")
        (field (name "LCSC") "C22961")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF2203T5E"))
      (property (name "LCSC") (value "C22961"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "3332d124-1bcb-4459-9e42-da7bb6e9a74c"))
    (comp (ref "R5")
      (value "51k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF5102T5E")
        (field (name "LCSC") "C23196")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF5102T5E"))
      (property (name "LCSC") (value "C23196"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "c85069bb-73b1-43ba-812c-8f7ab29d1350"))
    (comp (ref "R6")
      (value "330")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF3300T5E")
        (field (name "LCSC") "C23138")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF3300T5E"))
      (property (name "LCSC") (value "C23138"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "b76312c8-ca3f-4878-a259-ae5c42f10a6d"))
    (comp (ref "R7")
      (value "51k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF5102T5E")
        (field (name "LCSC") "C23196")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF5102T5E"))
      (property (name "LCSC") (value "C23196"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "9aa9887d-8762-4334-9cd6-b0b1bb251699"))
    (comp (ref "R8")
      (value "220k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF2203T5E")
        (field (name "LCSC") "C22961")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF2203T5E"))
      (property (name "LCSC") (value "C22961"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "36133e80-eb3e-418d-b27a-f47a8a15e83d"))
    (comp (ref "TP1")
      (value "TestPoint")
      (footprint "TestPoint:TestPoint_Pad_D1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Manufacturer"))
        (field (name "Manufacturer PN"))
        (field (name "Footprint") "TestPoint:TestPoint_Pad_D1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Manufacturer") (value ""))
      (property (name "Manufacturer PN") (value ""))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "f9d4e96d-5745-439f-90a0-b346d3dffc71"))
    (comp (ref "TP2")
      (value "TestPoint")
      (footprint "TestPoint:TestPoint_Pad_D1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Manufacturer"))
        (field (name "Manufacturer PN"))
        (field (name "Footprint") "TestPoint:TestPoint_Pad_D1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Manufacturer") (value ""))
      (property (name "Manufacturer PN") (value ""))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "b3386c76-edca-46a0-b57e-edd366b8ea57"))
    (comp (ref "TP11")
      (value "TestPoint")
      (footprint "Connector_Wire:SolderWirePad_1x01_SMD_2x4mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "Connector_Wire:SolderWirePad_1x01_SMD_2x4mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "b28a1eee-2f08-4428-9b24-9acd0c866799"))
    (comp (ref "TP12")
      (value "TestPoint")
      (footprint "Connector_Wire:SolderWirePad_1x01_SMD_2x4mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "Connector_Wire:SolderWirePad_1x01_SMD_2x4mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "3216bfe7-08e0-4b83-bee1-5c29e57aafb0"))
    (comp (ref "TP13")
      (value "TestPoint")
      (footprint "Connector_Wire:SolderWirePad_1x01_SMD_2x4mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "Connector_Wire:SolderWirePad_1x01_SMD_2x4mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "68f29406-bf4f-4737-ba92-51d121ee515a"))
    (comp (ref "TP14")
      (value "TestPoint")
      (footprint "Connector_Wire:SolderWirePad_1x01_SMD_2x4mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "Connector_Wire:SolderWirePad_1x01_SMD_2x4mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "0bb620d4-c3fb-4c47-8281-592b3a96db94"))
    (comp (ref "U1")
      (value "MCP6042T-I/MS")
      (footprint "Package_SO:MSOP-8_3x3mm_P0.65mm")
      (datasheet "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf")
      (description "Dual, 1 MHz, 85µA, Rail-to-Rail input and output, MSOP-8")
      (fields
        (field (name "LCSC") "C627438")
        (field (name "Manufacturer") "Microchip")
        (field (name "Manufacturer PN") "MCP6042-I/MS")
        (field (name "Footprint") "Package_SO:MSOP-8_3x3mm_P0.65mm")
        (field (name "Datasheet") "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf")
        (field (name "Description") "Dual, 1 MHz, 85µA, Rail-to-Rail input and output, MSOP-8"))
      (libsource (lib "Amplifier_Operational") (part "MCP6L02x-xMS") (description "Dual, 1 MHz, 85µA, Rail-to-Rail input and output, MSOP-8"))
      (property (name "LCSC") (value "C627438"))
      (property (name "Manufacturer") (value "Microchip"))
      (property (name "Manufacturer PN") (value "MCP6042-I/MS"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "opamp vfa r2r rtr"))
      (property (name "ki_fp_filters") (value "MSOP*3x3mm*P0.65mm*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "0aa2307e-1521-4275-a630-00398fb3d41d" "0aa2307e-1521-4275-a630-00398fb3d41c" "0aa2307e-1521-4275-a630-00398fb3d41b"))
    (comp (ref "U2")
      (value "MCP6042T-I/MS")
      (footprint "Package_SO:MSOP-8_3x3mm_P0.65mm")
      (datasheet "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf")
      (description "Dual, 1 MHz, 85µA, Rail-to-Rail input and output, MSOP-8")
      (fields
        (field (name "LCSC") "C627438")
        (field (name "Manufacturer") "Microchip")
        (field (name "Manufacturer PN") "MCP6042-I/MS")
        (field (name "Footprint") "Package_SO:MSOP-8_3x3mm_P0.65mm")
        (field (name "Datasheet") "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf")
        (field (name "Description") "Dual, 1 MHz, 85µA, Rail-to-Rail input and output, MSOP-8"))
      (libsource (lib "Amplifier_Operational") (part "MCP6L02x-xMS") (description "Dual, 1 MHz, 85µA, Rail-to-Rail input and output, MSOP-8"))
      (property (name "LCSC") (value "C627438"))
      (property (name "Manufacturer") (value "Microchip"))
      (property (name "Manufacturer PN") (value "MCP6042-I/MS"))
      (property (name "Sheetname") (value "Load Cell Amp"))
      (property (name "Sheetfile") (value "Load_Cell_Amp.kicad_sch"))
      (property (name "ki_keywords") (value "opamp vfa r2r rtr"))
      (property (name "ki_fp_filters") (value "MSOP*3x3mm*P0.65mm*"))
      (sheetpath (names "/Project Architecture/Load Cell Amp/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/a5aa3c11-5084-4ea5-9da5-c9ff4a86f01f/"))
      (tstamps "a61a0e42-7f51-4bfb-8f50-9c7649feec25" "69c94eba-401a-4da1-9a83-d9e5c5ae991c" "32fae178-0263-4c90-b1a2-cab80ff254a6"))
    (comp (ref "C3")
      (value "100u")
      (footprint "Capacitor_SMD:C_1206_3216Metric")
      (datasheet "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL31A107MQHNNNE")
      (description "capacitor, small US symbol")
      (fields
        (field (name "LCSC") "C15008")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Manufacturer PN") "CL31A107MQHNNNE")
        (field (name "Footprint") "Capacitor_SMD:C_1206_3216Metric")
        (field (name "Datasheet") "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL31A107MQHNNNE")
        (field (name "Description") "capacitor, small US symbol"))
      (libsource (lib "Device") (part "C_Small_US") (description "capacitor, small US symbol"))
      (property (name "LCSC") (value "C15008"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Manufacturer PN") (value "CL31A107MQHNNNE"))
      (property (name "Sheetname") (value "BLE Controller"))
      (property (name "Sheetfile") (value "BLE_Controller.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Project Architecture/BLE Controller/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/9da43fd7-7a0a-403c-bf2c-ba67cd8fa669/"))
      (tstamps "93136a12-d32b-4e0a-8538-e5b29077f1bf"))
    (comp (ref "C4")
      (value "100u")
      (footprint "Capacitor_SMD:C_1206_3216Metric")
      (datasheet "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL31A107MQHNNNE")
      (description "capacitor, small US symbol")
      (fields
        (field (name "LCSC") "C15008")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Manufacturer PN") "CL31A107MQHNNNE")
        (field (name "Footprint") "Capacitor_SMD:C_1206_3216Metric")
        (field (name "Datasheet") "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL31A107MQHNNNE")
        (field (name "Description") "capacitor, small US symbol"))
      (libsource (lib "Device") (part "C_Small_US") (description "capacitor, small US symbol"))
      (property (name "LCSC") (value "C15008"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Manufacturer PN") (value "CL31A107MQHNNNE"))
      (property (name "Sheetname") (value "BLE Controller"))
      (property (name "Sheetfile") (value "BLE_Controller.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Project Architecture/BLE Controller/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/9da43fd7-7a0a-403c-bf2c-ba67cd8fa669/"))
      (tstamps "d82905e9-94c3-46d4-9ca8-8f26a543f123"))
    (comp (ref "L1")
      (value "10uH")
      (footprint "Inductor_SMD:L_0603_1608Metric")
      (datasheet "https://product.tdk.com/system/files/dam/doc/product/inductor/inductor/smd/catalog/inductor_commercial_decoupling_mlz1608_en.pdf")
      (description "Inductor, small symbol")
      (fields
        (field (name "Manufacturer") "TDK")
        (field (name "Manufacturer PN") "MLZ1608M100WT000")
        (field (name "LCSC") "C76798")
        (field (name "Footprint") "Inductor_SMD:L_0603_1608Metric")
        (field (name "Datasheet") "https://product.tdk.com/system/files/dam/doc/product/inductor/inductor/smd/catalog/inductor_commercial_decoupling_mlz1608_en.pdf")
        (field (name "Description") "Inductor, small symbol"))
      (libsource (lib "Device") (part "L_Small") (description "Inductor, small symbol"))
      (property (name "Manufacturer") (value "TDK"))
      (property (name "Manufacturer PN") (value "MLZ1608M100WT000"))
      (property (name "LCSC") (value "C76798"))
      (property (name "Sheetname") (value "BLE Controller"))
      (property (name "Sheetfile") (value "BLE_Controller.kicad_sch"))
      (property (name "ki_keywords") (value "inductor choke coil reactor magnetic"))
      (property (name "ki_fp_filters") (value "Choke_* *Coil* Inductor_* L_*"))
      (sheetpath (names "/Project Architecture/BLE Controller/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/9da43fd7-7a0a-403c-bf2c-ba67cd8fa669/"))
      (tstamps "457cf768-eead-438e-83e3-304d941327b4"))
    (comp (ref "R9")
      (value "10k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF1002T5E")
        (field (name "LCSC") "C25804")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF1002T5E"))
      (property (name "LCSC") (value "C25804"))
      (property (name "Sheetname") (value "BLE Controller"))
      (property (name "Sheetfile") (value "BLE_Controller.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/BLE Controller/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/9da43fd7-7a0a-403c-bf2c-ba67cd8fa669/"))
      (tstamps "a681eb8c-bf92-43dc-90f9-fdde2a4eef00"))
    (comp (ref "R10")
      (value "22")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF220JT5E")
        (field (name "LCSC") "C23345")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF220JT5E"))
      (property (name "LCSC") (value "C23345"))
      (property (name "Sheetname") (value "BLE Controller"))
      (property (name "Sheetfile") (value "BLE_Controller.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/BLE Controller/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/9da43fd7-7a0a-403c-bf2c-ba67cd8fa669/"))
      (tstamps "332831fa-4ca8-4bf7-bbf1-1f9d0d7f0379"))
    (comp (ref "R11")
      (value "22")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF220JT5E")
        (field (name "LCSC") "C23345")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF220JT5E"))
      (property (name "LCSC") (value "C23345"))
      (property (name "Sheetname") (value "BLE Controller"))
      (property (name "Sheetfile") (value "BLE_Controller.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/BLE Controller/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/9da43fd7-7a0a-403c-bf2c-ba67cd8fa669/"))
      (tstamps "314c30e7-873a-4eae-bf54-e61b9d65a7da"))
    (comp (ref "R12")
      (value "10k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF1002T5E")
        (field (name "LCSC") "C25804")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF1002T5E"))
      (property (name "LCSC") (value "C25804"))
      (property (name "Sheetname") (value "BLE Controller"))
      (property (name "Sheetfile") (value "BLE_Controller.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/BLE Controller/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/9da43fd7-7a0a-403c-bf2c-ba67cd8fa669/"))
      (tstamps "0f36fc1e-e36f-4bbd-b0c1-d147c3a40559"))
    (comp (ref "R13")
      (value "10k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF1002T5E")
        (field (name "LCSC") "C25804")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF1002T5E"))
      (property (name "LCSC") (value "C25804"))
      (property (name "Sheetname") (value "BLE Controller"))
      (property (name "Sheetfile") (value "BLE_Controller.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/BLE Controller/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/9da43fd7-7a0a-403c-bf2c-ba67cd8fa669/"))
      (tstamps "c82cb63c-c096-4a91-9538-24f637845e62"))
    (comp (ref "U3")
      (value "MDBT50Q-1MV2")
      (footprint "RF_Module:Raytac_MDBT50Q")
      (datasheet "https://www.raytac.com/download/index.php?index_id=43")
      (description "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module")
      (fields
        (field (name "Manufacturer") "Raytac")
        (field (name "Manufacturer PN") "MDBT50Q-1MV2")
        (field (name "LCSC") "C5118826")
        (field (name "Footprint") "RF_Module:Raytac_MDBT50Q")
        (field (name "Datasheet") "https://www.raytac.com/download/index.php?index_id=43")
        (field (name "Description") "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module"))
      (libsource (lib "RF_Module") (part "MDBT50Q-1MV2") (description "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module"))
      (property (name "Manufacturer") (value "Raytac"))
      (property (name "Manufacturer PN") (value "MDBT50Q-1MV2"))
      (property (name "LCSC") (value "C5118826"))
      (property (name "Sheetname") (value "BLE Controller"))
      (property (name "Sheetfile") (value "BLE_Controller.kicad_sch"))
      (property (name "ki_keywords") (value "BLE ANT ZigBee Thread 802.15.4 nRF52840 nordic MDBT50Q"))
      (property (name "ki_fp_filters") (value "Raytac?MDBT50Q*"))
      (sheetpath (names "/Project Architecture/BLE Controller/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/9da43fd7-7a0a-403c-bf2c-ba67cd8fa669/"))
      (tstamps "147209bc-c059-460d-8034-8f6210941d23"))
    (comp (ref "C5")
      (value "1u")
      (footprint "Capacitor_SMD:C_0603_1608Metric")
      (datasheet "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL10A105KB8NNNC")
      (description "capacitor, small US symbol")
      (fields
        (field (name "LCSC") "C15849")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Manufacturer PN") "CL10A105KB8NNNC")
        (field (name "Footprint") "Capacitor_SMD:C_0603_1608Metric")
        (field (name "Datasheet") "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL10A105KB8NNNC")
        (field (name "Description") "capacitor, small US symbol"))
      (libsource (lib "Device") (part "C_Small_US") (description "capacitor, small US symbol"))
      (property (name "LCSC") (value "C15849"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Manufacturer PN") (value "CL10A105KB8NNNC"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "2f1e9155-c81c-4da7-9e9f-5a4f61426e04"))
    (comp (ref "C6")
      (value "2.2u")
      (footprint "Capacitor_SMD:C_0603_1608Metric")
      (datasheet "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL10A225KO8NNN")
      (description "capacitor, small US symbol")
      (fields
        (field (name "LCSC") "C23630")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Manufacturer PN") "CL10A225KO8NNNC")
        (field (name "Footprint") "Capacitor_SMD:C_0603_1608Metric")
        (field (name "Datasheet") "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL10A225KO8NNN")
        (field (name "Description") "capacitor, small US symbol"))
      (libsource (lib "Device") (part "C_Small_US") (description "capacitor, small US symbol"))
      (property (name "LCSC") (value "C23630"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Manufacturer PN") (value "CL10A225KO8NNNC"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "c93ffeff-50d5-463f-b756-5298c92ef9bf"))
    (comp (ref "C7")
      (value "4.7u")
      (footprint "Capacitor_SMD:C_0603_1608Metric")
      (datasheet "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL10A475KO8NNNC")
      (description "capacitor, small US symbol")
      (fields
        (field (name "LCSC") "C19666")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Manufacturer PN") "CL10A475KO8NNNC")
        (field (name "Footprint") "Capacitor_SMD:C_0603_1608Metric")
        (field (name "Datasheet") "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL10A475KO8NNNC")
        (field (name "Description") "capacitor, small US symbol"))
      (libsource (lib "Device") (part "C_Small_US") (description "capacitor, small US symbol"))
      (property (name "LCSC") (value "C19666"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Manufacturer PN") (value "CL10A475KO8NNNC"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "fdd4e32d-d0b4-4787-8783-8284de30f2d6"))
    (comp (ref "C8")
      (value "4.7u")
      (footprint "Capacitor_SMD:C_0603_1608Metric")
      (datasheet "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL10A475KO8NNNC")
      (description "capacitor, small US symbol")
      (fields
        (field (name "LCSC") "C19666")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Manufacturer PN") "CL10A475KO8NNNC")
        (field (name "Footprint") "Capacitor_SMD:C_0603_1608Metric")
        (field (name "Datasheet") "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL10A475KO8NNNC")
        (field (name "Description") "capacitor, small US symbol"))
      (libsource (lib "Device") (part "C_Small_US") (description "capacitor, small US symbol"))
      (property (name "LCSC") (value "C19666"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Manufacturer PN") (value "CL10A475KO8NNNC"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "bd667dbb-5d74-4434-a17f-782cf18168c3"))
    (comp (ref "J1")
      (value "B2B-PH-K")
      (footprint "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical")
      (datasheet "https://www.jst.com/wp-content/uploads/2025/06/ePH.pdf")
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Asymworks IPN"))
        (field (name "Manufacturer") "JST")
        (field (name "Manufacturer PN") "S2B-PH-SM4-TB")
        (field (name "LCSC") "C295747")
        (field (name "Footprint") "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical")
        (field (name "Datasheet") "https://www.jst.com/wp-content/uploads/2025/06/ePH.pdf")
        (field (name "Description") "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x02") (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Asymworks IPN") (value ""))
      (property (name "Manufacturer") (value "JST"))
      (property (name "Manufacturer PN") (value "S2B-PH-SM4-TB"))
      (property (name "LCSC") (value "C295747"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "50dbb54b-ac71-430d-9a54-934961ba73f0"))
    (comp (ref "J2")
      (value "B5B-PH-K")
      (footprint "Connector_JST:JST_PH_B5B-PH-K_1x05_P2.00mm_Vertical")
      (datasheet "https://www.jst.com/wp-content/uploads/2025/06/ePH.pdf")
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Asymworks IPN"))
        (field (name "Manufacturer") "JST")
        (field (name "Manufacturer PN") "S5B-PH-SM4-TB")
        (field (name "LCSC") "C265104")
        (field (name "Footprint") "Connector_JST:JST_PH_B5B-PH-K_1x05_P2.00mm_Vertical")
        (field (name "Datasheet") "https://www.jst.com/wp-content/uploads/2025/06/ePH.pdf")
        (field (name "Description") "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x05") (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Asymworks IPN") (value ""))
      (property (name "Manufacturer") (value "JST"))
      (property (name "Manufacturer PN") (value "S5B-PH-SM4-TB"))
      (property (name "LCSC") (value "C265104"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "3a474dca-bf00-4fba-8294-1d2e20569ac4"))
    (comp (ref "J3")
      (value "Conn_ARM_JTAG_SWD_10")
      (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD")
      (datasheet "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf")
      (description "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface")
      (fields
        (field (name "LCSC") "C150517")
        (field (name "Manufacturer") "Amphenol ICC")
        (field (name "Manufacturer PN") "20021121-00010C4LF")
        (field (name "Footprint") "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD")
        (field (name "Datasheet") "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf")
        (field (name "Description") "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface"))
      (libsource (lib "Connector") (part "Conn_ARM_JTAG_SWD_10") (description "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface"))
      (property (name "LCSC") (value "C150517"))
      (property (name "Manufacturer") (value "Amphenol ICC"))
      (property (name "Manufacturer PN") (value "20021121-00010C4LF"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "Cortex Debug Connector ARM SWD JTAG"))
      (property (name "ki_fp_filters") (value "PinHeader?2x05?P1.27mm*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "161d7b6a-da88-4f78-aa04-5fc04ec8537a"))
    (comp (ref "Q2")
      (value "Si2301CDS")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "https://www.vishay.com/doc/?68741")
      (description "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23")
      (fields
        (field (name "Manufacturer") "Vishay")
        (field (name "Manufacturer PN") "Si2301CDS-T1-GE3")
        (field (name "LCSC") "C10487")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "https://www.vishay.com/doc/?68741")
        (field (name "Description") "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23"))
      (libsource (lib "Asym_Transistor_FET") (part "Si2301CDS") (description "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23"))
      (property (name "Manufacturer") (value "Vishay"))
      (property (name "Manufacturer PN") (value "Si2301CDS-T1-GE3"))
      (property (name "LCSC") (value "C10487"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "P-Channel MOSFET"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "df33d6d6-fa23-43f5-b866-ef3bda05fc2c"))
    (comp (ref "Q3")
      (value "Si2301CDS")
      (footprint "Package_TO_SOT_SMD:SOT-23")
      (datasheet "https://www.vishay.com/doc/?68741")
      (description "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23")
      (fields
        (field (name "Manufacturer") "Vishay")
        (field (name "Manufacturer PN") "Si2301CDS-T1-GE3")
        (field (name "LCSC") "C10487")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "https://www.vishay.com/doc/?68741")
        (field (name "Description") "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23"))
      (libsource (lib "Asym_Transistor_FET") (part "Si2301CDS") (description "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23"))
      (property (name "Manufacturer") (value "Vishay"))
      (property (name "Manufacturer PN") (value "Si2301CDS-T1-GE3"))
      (property (name "LCSC") (value "C10487"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "P-Channel MOSFET"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "560bbe63-941a-439d-9c3a-536aa7695322"))
    (comp (ref "R14")
      (value "75")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF750JT5E")
        (field (name "LCSC") "C4275")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF750JT5E"))
      (property (name "LCSC") (value "C4275"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "bddee7e6-cd4d-443c-9676-358ec0511217"))
    (comp (ref "R15")
      (value "10k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF1002T5E")
        (field (name "LCSC") "C25804")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF1002T5E"))
      (property (name "LCSC") (value "C25804"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "a10878da-6a82-4965-9cf9-8591f8d0394c"))
    (comp (ref "R16")
      (value "10k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF1002T5E")
        (field (name "LCSC") "C25804")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF1002T5E"))
      (property (name "LCSC") (value "C25804"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "2385ef7a-d010-4dbf-a557-70853284825b"))
    (comp (ref "R17")
      (value "5.1k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF5101T5E")
        (field (name "LCSC") "C23186")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF5101T5E"))
      (property (name "LCSC") (value "C23186"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "9aa71257-d96e-4aee-a72f-042865c65129"))
    (comp (ref "R18")
      (value "220")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF2200T5E")
        (field (name "LCSC") "C22962")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF2200T5E"))
      (property (name "LCSC") (value "C22962"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "54468572-129f-4dd2-ac51-b2a29d50802c"))
    (comp (ref "R19")
      (value "10k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF1002T5E")
        (field (name "LCSC") "C25804")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF1002T5E"))
      (property (name "LCSC") (value "C25804"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "f4e06be6-aa8b-431e-818f-ef982fd2f17f"))
    (comp (ref "R20")
      (value "10k")
      (footprint "Resistor_SMD:R_0603_1608Metric")
      (datasheet "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
      (description "Resistor, US symbol")
      (fields
        (field (name "Manufacturer") "Uni-Royal")
        (field (name "Manufacturer PN") "0603WAF1002T5E")
        (field (name "LCSC") "C25804")
        (field (name "Footprint") "Resistor_SMD:R_0603_1608Metric")
        (field (name "Datasheet") "https://www.royalohm.com/assets/pdf/products/smd/1.pdf")
        (field (name "Description") "Resistor, US symbol"))
      (libsource (lib "Device") (part "R_US") (description "Resistor, US symbol"))
      (property (name "Manufacturer") (value "Uni-Royal"))
      (property (name "Manufacturer PN") (value "0603WAF1002T5E"))
      (property (name "LCSC") (value "C25804"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "bbbfc804-fd6d-417a-ab69-ebb4605dd3e4"))
    (comp (ref "TP3")
      (value "TestPoint")
      (footprint "TestPoint:TestPoint_Pad_D1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Manufacturer"))
        (field (name "Manufacturer PN"))
        (field (name "Footprint") "TestPoint:TestPoint_Pad_D1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Manufacturer") (value ""))
      (property (name "Manufacturer PN") (value ""))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "a1cce5a3-27bf-4bda-b8cc-f131b92cc56c"))
    (comp (ref "TP4")
      (value "TestPoint")
      (footprint "TestPoint:TestPoint_Pad_D1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Manufacturer"))
        (field (name "Manufacturer PN"))
        (field (name "Footprint") "TestPoint:TestPoint_Pad_D1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Manufacturer") (value ""))
      (property (name "Manufacturer PN") (value ""))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "a64e2846-e0ef-472d-be8a-2a14e8424886"))
    (comp (ref "TP5")
      (value "TestPoint")
      (footprint "TestPoint:TestPoint_Pad_D1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Manufacturer"))
        (field (name "Manufacturer PN"))
        (field (name "Footprint") "TestPoint:TestPoint_Pad_D1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Manufacturer") (value ""))
      (property (name "Manufacturer PN") (value ""))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "3167e078-6056-472d-893c-50dff7c00c71"))
    (comp (ref "TP6")
      (value "TestPoint")
      (footprint "TestPoint:TestPoint_Pad_D1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Manufacturer"))
        (field (name "Manufacturer PN"))
        (field (name "Footprint") "TestPoint:TestPoint_Pad_D1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Manufacturer") (value ""))
      (property (name "Manufacturer PN") (value ""))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "b5b3a0fd-6550-417e-bb7b-b87d80c5451b"))
    (comp (ref "TP7")
      (value "TestPoint")
      (footprint "TestPoint:TestPoint_Pad_D1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Manufacturer"))
        (field (name "Manufacturer PN"))
        (field (name "Footprint") "TestPoint:TestPoint_Pad_D1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Manufacturer") (value ""))
      (property (name "Manufacturer PN") (value ""))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "a581c007-f3cd-4158-84e3-325d7bd83247"))
    (comp (ref "TP8")
      (value "TestPoint")
      (footprint "TestPoint:TestPoint_Pad_D1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Manufacturer"))
        (field (name "Manufacturer PN"))
        (field (name "Footprint") "TestPoint:TestPoint_Pad_D1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Manufacturer") (value ""))
      (property (name "Manufacturer PN") (value ""))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "3f0204d8-153c-4d58-8e9b-331f19382f8a"))
    (comp (ref "TP9")
      (value "TestPoint")
      (footprint "TestPoint:TestPoint_Pad_D1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Manufacturer"))
        (field (name "Manufacturer PN"))
        (field (name "Footprint") "TestPoint:TestPoint_Pad_D1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Manufacturer") (value ""))
      (property (name "Manufacturer PN") (value ""))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "9efe8f44-f06c-445d-93df-a1c0ee64bb5c"))
    (comp (ref "TP10")
      (value "TestPoint")
      (footprint "TestPoint:TestPoint_Pad_D1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Manufacturer"))
        (field (name "Manufacturer PN"))
        (field (name "Footprint") "TestPoint:TestPoint_Pad_D1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Manufacturer") (value ""))
      (property (name "Manufacturer PN") (value ""))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "a5a3296f-9044-41a6-ae46-69267e919f61"))
    (comp (ref "U4")
      (value "BQ27427")
      (footprint "Package_BGA:Texas_DSBGA-9_1.62x1.58mm_Layout3x3_P0.5mm")
      (datasheet "https://www.ti.com/lit/ds/symlink/bq27427.pdf")
      (description "Li-Ion/Li-Po battery monitor and fuel guage")
      (fields
        (field (name "Manufacturer") "Texas Instruments")
        (field (name "Manufacturer PN") "BQ27427YZFR")
        (field (name "LCSC") "C6075475")
        (field (name "Footprint") "Package_BGA:Texas_DSBGA-9_1.62x1.58mm_Layout3x3_P0.5mm")
        (field (name "Datasheet") "https://www.ti.com/lit/ds/symlink/bq27427.pdf")
        (field (name "Description") "Li-Ion/Li-Po battery monitor and fuel guage"))
      (libsource (lib "Asym_Battery_Management") (part "BQ27427") (description ""))
      (property (name "Manufacturer") (value "Texas Instruments"))
      (property (name "Manufacturer PN") (value "BQ27427YZFR"))
      (property (name "LCSC") (value "C6075475"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "Single-Cell Battery Fuel Guage with Integrated Sense Resistor"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "0063a907-4a81-4dcf-a838-8131cfa40f99"))
    (comp (ref "U5")
      (value "MCP73832T-2ACI/OT")
      (footprint "Package_TO_SOT_SMD:SOT-23-5")
      (datasheet "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf")
      (description "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Tri-State Status Output, in SOT23-5 package")
      (fields
        (field (name "LCSC") "C424093")
        (field (name "Manufacturer") "Microchip")
        (field (name "Manufacturer PN") "MCP73832T-2ACI/OT")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23-5")
        (field (name "Datasheet") "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf")
        (field (name "Description") "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Tri-State Status Output, in SOT23-5 package"))
      (libsource (lib "Battery_Management") (part "MCP73831-2-OT") (description "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Tri-State Status Output, in SOT23-5 package"))
      (property (name "LCSC") (value "C424093"))
      (property (name "Manufacturer") (value "Microchip"))
      (property (name "Manufacturer PN") (value "MCP73832T-2ACI/OT"))
      (property (name "Sheetname") (value "Power and Interface"))
      (property (name "Sheetfile") (value "Power_Interface.kicad_sch"))
      (property (name "ki_keywords") (value "battery charger lithium"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/Project Architecture/Power and Interface/") (tstamps "/f6afef58-d841-4ad6-baf9-746b0a35f011/6c8ce547-8e28-496a-9003-0e7dbfd93e8c/"))
      (tstamps "c214e3e9-6415-4922-8a06-e1a32697a8b6")))
  (libparts
    (libpart (lib "Amplifier_Operational") (part "MCP6L02x-xMS")
      (description "Dual, 1 MHz, 85µA, Rail-to-Rail input and output, MSOP-8")
      (docs "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf")
      (footprints
        (fp "MSOP*3x3mm*P0.65mm*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "MCP6L02x-xMS")
        (field (name "Footprint") "Package_SO:MSOP-8_3x3mm_P0.65mm")
        (field (name "Datasheet") "http://ww1.microchip.com/downloads/en/devicedoc/22140b.pdf")
        (field (name "Description") "Dual, 1 MHz, 85µA, Rail-to-Rail input and output, MSOP-8"))
      (pins
        (pin (num "1") (name "") (type "output"))
        (pin (num "2") (name "-") (type "input"))
        (pin (num "3") (name "+") (type "input"))
        (pin (num "4") (name "V-") (type "power_in"))
        (pin (num "5") (name "+") (type "input"))
        (pin (num "6") (name "-") (type "input"))
        (pin (num "7") (name "") (type "output"))
        (pin (num "8") (name "V+") (type "power_in"))))
    (libpart (lib "Asym_Battery_Management") (part "BQ27427")
      (docs "https://www.ti.com/lit/ds/symlink/bq27427.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "BQ27427")
        (field (name "Footprint") "Package_BGA:Texas_DSBGA-9_1.62x1.58mm_Layout3x3_P0.5mm")
        (field (name "Datasheet") "https://www.ti.com/lit/ds/symlink/bq27427.pdf")
        (field (name "Description")))
      (pins
        (pin (num "A1") (name "GPOUT") (type "open_collector"))
        (pin (num "A2") (name "SDA") (type "bidirectional"))
        (pin (num "A3") (name "SCL") (type "input"))
        (pin (num "B1") (name "BIN") (type "input"))
        (pin (num "B2") (name "VSS") (type "power_out"))
        (pin (num "B3") (name "VDD") (type "power_out"))
        (pin (num "C1") (name "VSS") (type "power_out"))
        (pin (num "C2") (name "SRX") (type "power_in"))
        (pin (num "C3") (name "BAT") (type "power_in"))))
    (libpart (lib "Asym_Transistor_FET") (part "Si2301CDS")
      (description "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23")
      (docs "https://www.vishay.com/doc/?68741")
      (fields
        (field (name "Reference") "Q")
        (field (name "Value") "Si2301CDS")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23")
        (field (name "Datasheet") "https://www.vishay.com/doc/?68741")
        (field (name "Description") "-3.1A Id, -20V Vds, P-Channel MOSFET, SOT-23"))
      (pins
        (pin (num "1") (name "G") (type "input"))
        (pin (num "2") (name "S") (type "passive"))
        (pin (num "3") (name "D") (type "passive"))))
    (libpart (lib "Battery_Management") (part "MCP73831-2-OT")
      (description "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Tri-State Status Output, in SOT23-5 package")
      (docs "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf")
      (footprints
        (fp "SOT?23*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "MCP73831-2-OT")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23-5")
        (field (name "Datasheet") "http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf")
        (field (name "Description") "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Tri-State Status Output, in SOT23-5 package"))
      (pins
        (pin (num "1") (name "STAT") (type "tri_state"))
        (pin (num "2") (name "V_{SS}") (type "power_in"))
        (pin (num "3") (name "V_{BAT}") (type "power_out"))
        (pin (num "4") (name "V_{DD}") (type "power_in"))
        (pin (num "5") (name "PROG") (type "input"))))
    (libpart (lib "Connector") (part "Conn_ARM_JTAG_SWD_10")
      (description "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface")
      (docs "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf")
      (footprints
        (fp "PinHeader?2x05?P1.27mm*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_ARM_JTAG_SWD_10")
        (field (name "Footprint"))
        (field (name "Datasheet") "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf")
        (field (name "Description") "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface"))
      (pins
        (pin (num "1") (name "VTref") (type "power_in"))
        (pin (num "2") (name "SWDIO/TMS") (type "bidirectional"))
        (pin (num "3") (name "GND") (type "power_in"))
        (pin (num "4") (name "SWCLK/TCK") (type "output"))
        (pin (num "5") (name "GND") (type "passive"))
        (pin (num "6") (name "SWO/TDO") (type "input"))
        (pin (num "7") (name "KEY") (type "no_connect"))
        (pin (num "8") (name "NC/TDI") (type "output"))
        (pin (num "9") (name "GNDDetect") (type "passive"))
        (pin (num "10") (name "~{RESET}") (type "open_collector"))))
    (libpart (lib "Connector") (part "TestPoint")
      (description "test point")
      (docs "~")
      (footprints
        (fp "Pin*")
        (fp "Test*"))
      (fields
        (field (name "Reference") "TP")
        (field (name "Value") "TestPoint")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (pins
        (pin (num "1") (name "1") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x02")
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x02")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x05")
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x05")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))))
    (libpart (lib "Device") (part "C_Small_US")
      (description "capacitor, small US symbol")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "C_Small_US")
        (field (name "Footprint"))
        (field (name "Datasheet"))
        (field (name "Description") "capacitor, small US symbol"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Device") (part "L_Small")
      (description "Inductor, small symbol")
      (docs "~")
      (footprints
        (fp "Choke_*")
        (fp "*Coil*")
        (fp "Inductor_*")
        (fp "L_*"))
      (fields
        (field (name "Reference") "L")
        (field (name "Value") "L_Small")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Inductor, small symbol"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Device") (part "R_US")
      (description "Resistor, US symbol")
      (docs "~")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "R_US")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor, US symbol"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "RF_Module") (part "MDBT50Q-1MV2")
      (description "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module")
      (docs "https://www.raytac.com/download/index.php?index_id=43")
      (footprints
        (fp "Raytac?MDBT50Q*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "MDBT50Q-1MV2")
        (field (name "Footprint") "RF_Module:Raytac_MDBT50Q")
        (field (name "Datasheet") "https://www.raytac.com/download/index.php?index_id=43")
        (field (name "Description") "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52840 module"))
      (pins
        (pin (num "1") (name "GND") (type "power_in"))
        (pin (num "2") (name "GND") (type "passive"))
        (pin (num "3") (name "P1.10") (type "bidirectional"))
        (pin (num "4") (name "P1.11") (type "bidirectional"))
        (pin (num "5") (name "P1.12") (type "bidirectional"))
        (pin (num "6") (name "P1.13") (type "bidirectional"))
        (pin (num "7") (name "P1.14") (type "bidirectional"))
        (pin (num "8") (name "P1.15") (type "bidirectional"))
        (pin (num "9") (name "P0.03") (type "bidirectional"))
        (pin (num "10") (name "P0.29") (type "bidirectional"))
        (pin (num "11") (name "P0.02") (type "bidirectional"))
        (pin (num "12") (name "P0.31") (type "bidirectional"))
        (pin (num "13") (name "P0.28") (type "bidirectional"))
        (pin (num "14") (name "P0.30") (type "bidirectional"))
        (pin (num "15") (name "GND") (type "passive"))
        (pin (num "16") (name "P0.27") (type "bidirectional"))
        (pin (num "17") (name "P0.00") (type "bidirectional"))
        (pin (num "18") (name "P0.01") (type "bidirectional"))
        (pin (num "19") (name "P0.26") (type "bidirectional"))
        (pin (num "20") (name "P0.04") (type "bidirectional"))
        (pin (num "21") (name "P0.05") (type "bidirectional"))
        (pin (num "22") (name "P0.06") (type "bidirectional"))
        (pin (num "23") (name "P0.07") (type "bidirectional"))
        (pin (num "24") (name "P0.08") (type "bidirectional"))
        (pin (num "25") (name "P1.08") (type "bidirectional"))
        (pin (num "26") (name "P1.09") (type "bidirectional"))
        (pin (num "27") (name "P0.11") (type "bidirectional"))
        (pin (num "28") (name "VDD") (type "power_in"))
        (pin (num "29") (name "P0.12") (type "bidirectional"))
        (pin (num "30") (name "VDDH") (type "power_in"))
        (pin (num "31") (name "DCCH") (type "power_out"))
        (pin (num "32") (name "VBUS") (type "power_in"))
        (pin (num "33") (name "GND") (type "passive"))
        (pin (num "34") (name "D-") (type "bidirectional"))
        (pin (num "35") (name "D+") (type "bidirectional"))
        (pin (num "36") (name "P0.14") (type "bidirectional"))
        (pin (num "37") (name "P0.13") (type "bidirectional"))
        (pin (num "38") (name "P0.16") (type "bidirectional"))
        (pin (num "39") (name "P0.15") (type "bidirectional"))
        (pin (num "40") (name "P0.18") (type "bidirectional"))
        (pin (num "41") (name "P0.17") (type "bidirectional"))
        (pin (num "42") (name "P0.19") (type "bidirectional"))
        (pin (num "43") (name "P0.21") (type "bidirectional"))
        (pin (num "44") (name "P0.20") (type "bidirectional"))
        (pin (num "45") (name "P0.23") (type "bidirectional"))
        (pin (num "46") (name "P0.22") (type "bidirectional"))
        (pin (num "47") (name "P1.00") (type "bidirectional"))
        (pin (num "48") (name "P0.24") (type "bidirectional"))
        (pin (num "49") (name "P0.25") (type "bidirectional"))
        (pin (num "50") (name "P1.02") (type "bidirectional"))
        (pin (num "51") (name "SWDIO") (type "bidirectional"))
        (pin (num "52") (name "P0.09") (type "bidirectional"))
        (pin (num "53") (name "SWDCLK") (type "input"))
        (pin (num "54") (name "P0.10") (type "bidirectional"))
        (pin (num "55") (name "GND") (type "passive"))
        (pin (num "56") (name "P1.04") (type "bidirectional"))
        (pin (num "57") (name "P1.06") (type "bidirectional"))
        (pin (num "58") (name "P1.07") (type "bidirectional"))
        (pin (num "59") (name "P1.05") (type "bidirectional"))
        (pin (num "60") (name "P1.03") (type "bidirectional"))
        (pin (num "61") (name "P1.01") (type "bidirectional")))))
  (libraries
    (library (logical "Asym_Battery_Management")
      (uri "/workspace/jkrauss/Test_5/lib/asymworks/symbols/Asym_Battery_Management.kicad_sym"))
    (library (logical "Asym_Transistor_FET")
      (uri "/workspace/jkrauss/Test_5/lib/asymworks/symbols/Asym_Transistor_FET.kicad_sym")))
  (nets
    (net (code "1") (name "+3.3V") (class "Default")
      (node (ref "C1") (pin "1") (pintype "passive"))
      (node (ref "C2") (pin "1") (pintype "passive"))
      (node (ref "C4") (pin "1") (pintype "passive"))
      (node (ref "J3") (pin "1") (pinfunction "VTref") (pintype "power_in"))
      (node (ref "L1") (pin "1") (pintype "passive"))
      (node (ref "Q1") (pin "3") (pinfunction "D") (pintype "passive"))
      (node (ref "R1") (pin "1") (pintype "passive"))
      (node (ref "R12") (pin "1") (pintype "passive"))
      (node (ref "R13") (pin "1") (pintype "passive"))
      (node (ref "R16") (pin "1") (pintype "passive"))
      (node (ref "R19") (pin "1") (pintype "passive"))
      (node (ref "R2") (pin "2") (pintype "passive"))
      (node (ref "R20") (pin "1") (pintype "passive"))
      (node (ref "R9") (pin "1") (pintype "passive"))
      (node (ref "TP8") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "8") (pinfunction "V+") (pintype "power_in"))
      (node (ref "U2") (pin "8") (pinfunction "V+") (pintype "power_in"))
      (node (ref "U3") (pin "28") (pinfunction "VDD") (pintype "power_in")))
    (net (code "2") (name "/Project Architecture/BLE Controller/LOAD_CELL") (class "Default")
      (node (ref "R8") (pin "1") (pintype "passive"))
      (node (ref "TP2") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U2") (pin "7") (pintype "output"))
      (node (ref "U3") (pin "20") (pinfunction "P0.04") (pintype "bidirectional")))
    (net (code "3") (name "/Project Architecture/BLE Controller/SCL") (class "Default")
      (node (ref "R13") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "27") (pinfunction "P0.11") (pintype "bidirectional"))
      (node (ref "U4") (pin "A3") (pinfunction "SCL") (pintype "input")))
    (net (code "4") (name "/Project Architecture/BLE Controller/SDA") (class "Default")
      (node (ref "R12") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "29") (pinfunction "P0.12") (pintype "bidirectional"))
      (node (ref "U4") (pin "A2") (pinfunction "SDA") (pintype "bidirectional")))
    (net (code "5") (name "/Project Architecture/BLE Controller/~{BATT_INT}") (class "Default")
      (node (ref "R20") (pin "2") (pintype "passive"))
      (node (ref "TP4") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U3") (pin "16") (pinfunction "P0.27") (pintype "bidirectional"))
      (node (ref "U4") (pin "A1") (pinfunction "GPOUT") (pintype "open_collector")))
    (net (code "6") (name "/Project Architecture/BLE Controller/~{LOAD_CELL_EN}") (class "Default")
      (node (ref "Q1") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "R1") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "4") (pinfunction "P1.11") (pintype "bidirectional")))
    (net (code "7") (name "/Project Architecture/BLE Controller/~{PAIR_LED}") (class "Default")
      (node (ref "Q3") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "R19") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "50") (pinfunction "P1.02") (pintype "bidirectional")))
    (net (code "8") (name "/Project Architecture/BLE Controller/~{PAIR_SW}") (class "Default")
      (node (ref "J2") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "R9") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "44") (pinfunction "P0.20") (pintype "bidirectional")))
    (net (code "9") (name "/Project Architecture/Load Cell Amp/EXC+") (class "Default")
      (node (ref "Q1") (pin "2") (pinfunction "S") (pintype "passive"))
      (node (ref "TP11") (pin "1") (pinfunction "1") (pintype "passive")))
    (net (code "10") (name "/Project Architecture/Load Cell Amp/SIG+") (class "Default")
      (node (ref "TP13") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U2") (pin "3") (pinfunction "+") (pintype "input")))
    (net (code "11") (name "/Project Architecture/Load Cell Amp/SIG-") (class "Default")
      (node (ref "TP14") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U2") (pin "5") (pinfunction "+") (pintype "input")))
    (net (code "12") (name "/Project Architecture/Power and Interface/CHARGE_LED_IO") (class "Default")
      (node (ref "J2") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "R14") (pin "2") (pintype "passive")))
    (net (code "13") (name "/Project Architecture/Power and Interface/PAIR_LED_IO") (class "Default")
      (node (ref "J2") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "R18") (pin "2") (pintype "passive")))
    (net (code "14") (name "/Project Architecture/Power and Interface/STAT") (class "Default")
      (node (ref "Q2") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "R16") (pin "2") (pintype "passive"))
      (node (ref "TP5") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U3") (pin "36") (pinfunction "P0.14") (pintype "bidirectional"))
      (node (ref "U5") (pin "1") (pinfunction "STAT") (pintype "tri_state")))
    (net (code "15") (name "/Project Architecture/Power and Interface/SWDCLK") (class "Default")
      (node (ref "J3") (pin "4") (pinfunction "SWCLK/TCK") (pintype "output"))
      (node (ref "R11") (pin "1") (pintype "passive"))
      (node (ref "TP7") (pin "1") (pinfunction "1") (pintype "passive")))
    (net (code "16") (name "/Project Architecture/Power and Interface/SWDIO") (class "Default")
      (node (ref "J3") (pin "2") (pinfunction "SWDIO/TMS") (pintype "bidirectional"))
      (node (ref "R10") (pin "1") (pintype "passive"))
      (node (ref "TP10") (pin "1") (pinfunction "1") (pintype "passive")))
    (net (code "17") (name "/Project Architecture/Power and Interface/~{RESET}") (class "Default")
      (node (ref "J3") (pin "10") (pinfunction "~{RESET}") (pintype "open_collector"))
      (node (ref "TP6") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U3") (pin "40") (pinfunction "P0.18") (pintype "bidirectional")))
    (net (code "18") (name "GND") (class "Default")
      (node (ref "C1") (pin "2") (pintype "passive"))
      (node (ref "C2") (pin "2") (pintype "passive"))
      (node (ref "C3") (pin "2") (pintype "passive"))
      (node (ref "C4") (pin "2") (pintype "passive"))
      (node (ref "C5") (pin "2") (pintype "passive"))
      (node (ref "C6") (pin "2") (pintype "passive"))
      (node (ref "C7") (pin "2") (pintype "passive"))
      (node (ref "C8") (pin "2") (pintype "passive"))
      (node (ref "J1") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "J2") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "J3") (pin "3") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J3") (pin "5") (pinfunction "GND") (pintype "passive"))
      (node (ref "J3") (pin "9") (pinfunction "GNDDetect") (pintype "passive"))
      (node (ref "R15") (pin "2") (pintype "passive"))
      (node (ref "R17") (pin "2") (pintype "passive"))
      (node (ref "R3") (pin "1") (pintype "passive"))
      (node (ref "TP12") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "TP9") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "4") (pinfunction "V-") (pintype "power_in"))
      (node (ref "U1") (pin "5") (pinfunction "+") (pintype "input"))
      (node (ref "U2") (pin "4") (pinfunction "V-") (pintype "power_in"))
      (node (ref "U3") (pin "1") (pinfunction "GND") (pintype "power_in"))
      (node (ref "U3") (pin "15") (pinfunction "GND") (pintype "passive"))
      (node (ref "U3") (pin "2") (pinfunction "GND") (pintype "passive"))
      (node (ref "U3") (pin "33") (pinfunction "GND") (pintype "passive"))
      (node (ref "U3") (pin "55") (pinfunction "GND") (pintype "passive"))
      (node (ref "U4") (pin "B2") (pinfunction "VSS") (pintype "power_out"))
      (node (ref "U4") (pin "C1") (pinfunction "VSS") (pintype "power_out"))
      (node (ref "U5") (pin "2") (pinfunction "V_{SS}") (pintype "power_in")))
    (net (code "19") (name "Net-(J1-Pin_1)") (class "Default")
      (node (ref "C5") (pin "1") (pintype "passive"))
      (node (ref "J1") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "TP3") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U4") (pin "C3") (pinfunction "BAT") (pintype "power_in")))
    (net (code "20") (name "Net-(Q2-S)") (class "Default")
      (node (ref "Q2") (pin "2") (pinfunction "S") (pintype "passive"))
      (node (ref "R14") (pin "1") (pintype "passive")))
    (net (code "21") (name "Net-(Q3-S)") (class "Default")
      (node (ref "Q3") (pin "2") (pinfunction "S") (pintype "passive"))
      (node (ref "R18") (pin "1") (pintype "passive")))
    (net (code "22") (name "Net-(R5-Pad1)") (class "Default")
      (node (ref "R5") (pin "1") (pintype "passive"))
      (node (ref "R7") (pin "2") (pintype "passive"))
      (node (ref "U2") (pin "1") (pintype "output")))
    (net (code "23") (name "Net-(U1A-+)") (class "Default")
      (node (ref "R2") (pin "1") (pintype "passive"))
      (node (ref "R3") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "3") (pinfunction "+") (pintype "input")))
    (net (code "24") (name "Net-(U1A--)") (class "Default")
      (node (ref "R4") (pin "2") (pintype "passive"))
      (node (ref "TP1") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "1") (pintype "output"))
      (node (ref "U1") (pin "2") (pinfunction "-") (pintype "input")))
    (net (code "25") (name "Net-(U1B--)") (class "Default")
      (node (ref "U1") (pin "6") (pinfunction "-") (pintype "input"))
      (node (ref "U1") (pin "7") (pintype "output")))
    (net (code "26") (name "Net-(U2A--)") (class "Default")
      (node (ref "R4") (pin "1") (pintype "passive"))
      (node (ref "R5") (pin "2") (pintype "passive"))
      (node (ref "R6") (pin "2") (pintype "passive"))
      (node (ref "U2") (pin "2") (pinfunction "-") (pintype "input")))
    (net (code "27") (name "Net-(U2B--)") (class "Default")
      (node (ref "R6") (pin "1") (pintype "passive"))
      (node (ref "R7") (pin "1") (pintype "passive"))
      (node (ref "R8") (pin "2") (pintype "passive"))
      (node (ref "U2") (pin "6") (pinfunction "-") (pintype "input")))
    (net (code "28") (name "Net-(U3-DCCH)") (class "Default")
      (node (ref "L1") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "31") (pinfunction "DCCH") (pintype "power_out")))
    (net (code "29") (name "Net-(U3-SWDCLK)") (class "Default")
      (node (ref "R11") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "53") (pinfunction "SWDCLK") (pintype "input")))
    (net (code "30") (name "Net-(U3-SWDIO)") (class "Default")
      (node (ref "R10") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "51") (pinfunction "SWDIO") (pintype "bidirectional")))
    (net (code "31") (name "Net-(U4-BIN)") (class "Default")
      (node (ref "R15") (pin "1") (pintype "passive"))
      (node (ref "U4") (pin "B1") (pinfunction "BIN") (pintype "input")))
    (net (code "32") (name "Net-(U4-VDD)") (class "Default")
      (node (ref "C6") (pin "1") (pintype "passive"))
      (node (ref "U4") (pin "B3") (pinfunction "VDD") (pintype "power_out")))
    (net (code "33") (name "Net-(U5-PROG)") (class "Default")
      (node (ref "R17") (pin "1") (pintype "passive"))
      (node (ref "U5") (pin "5") (pinfunction "PROG") (pintype "input")))
    (net (code "34") (name "VBUS") (class "Default")
      (node (ref "C7") (pin "1") (pintype "passive"))
      (node (ref "J2") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U5") (pin "4") (pinfunction "V_{DD}") (pintype "power_in")))
    (net (code "35") (name "VDD") (class "Default")
      (node (ref "C3") (pin "1") (pintype "passive"))
      (node (ref "C8") (pin "1") (pintype "passive"))
      (node (ref "Q2") (pin "3") (pinfunction "D") (pintype "passive"))
      (node (ref "Q3") (pin "3") (pinfunction "D") (pintype "passive"))
      (node (ref "U3") (pin "30") (pinfunction "VDDH") (pintype "power_in"))
      (node (ref "U4") (pin "C2") (pinfunction "SRX") (pintype "power_in"))
      (node (ref "U5") (pin "3") (pinfunction "V_{BAT}") (pintype "power_out")))
    (net (code "36") (name "unconnected-(J3-KEY-Pad7)") (class "Default")
      (node (ref "J3") (pin "7") (pinfunction "KEY") (pintype "no_connect")))
    (net (code "37") (name "unconnected-(J3-NC{slash}TDI-Pad8)") (class "Default")
      (node (ref "J3") (pin "8") (pinfunction "NC/TDI") (pintype "output+no_connect")))
    (net (code "38") (name "unconnected-(J3-SWO{slash}TDO-Pad6)") (class "Default")
      (node (ref "J3") (pin "6") (pinfunction "SWO/TDO") (pintype "input+no_connect")))
    (net (code "39") (name "unconnected-(U3-D+-Pad35)") (class "Default")
      (node (ref "U3") (pin "35") (pinfunction "D+") (pintype "bidirectional+no_connect")))
    (net (code "40") (name "unconnected-(U3-D--Pad34)") (class "Default")
      (node (ref "U3") (pin "34") (pinfunction "D-") (pintype "bidirectional+no_connect")))
    (net (code "41") (name "unconnected-(U3-P0.00-Pad17)") (class "Default")
      (node (ref "U3") (pin "17") (pinfunction "P0.00") (pintype "bidirectional+no_connect")))
    (net (code "42") (name "unconnected-(U3-P0.01-Pad18)") (class "Default")
      (node (ref "U3") (pin "18") (pinfunction "P0.01") (pintype "bidirectional+no_connect")))
    (net (code "43") (name "unconnected-(U3-P0.02-Pad11)") (class "Default")
      (node (ref "U3") (pin "11") (pinfunction "P0.02") (pintype "bidirectional+no_connect")))
    (net (code "44") (name "unconnected-(U3-P0.03-Pad9)") (class "Default")
      (node (ref "U3") (pin "9") (pinfunction "P0.03") (pintype "bidirectional+no_connect")))
    (net (code "45") (name "unconnected-(U3-P0.05-Pad21)") (class "Default")
      (node (ref "U3") (pin "21") (pinfunction "P0.05") (pintype "bidirectional+no_connect")))
    (net (code "46") (name "unconnected-(U3-P0.06-Pad22)") (class "Default")
      (node (ref "U3") (pin "22") (pinfunction "P0.06") (pintype "bidirectional+no_connect")))
    (net (code "47") (name "unconnected-(U3-P0.07-Pad23)") (class "Default")
      (node (ref "U3") (pin "23") (pinfunction "P0.07") (pintype "bidirectional+no_connect")))
    (net (code "48") (name "unconnected-(U3-P0.08-Pad24)") (class "Default")
      (node (ref "U3") (pin "24") (pinfunction "P0.08") (pintype "bidirectional+no_connect")))
    (net (code "49") (name "unconnected-(U3-P0.09-Pad52)") (class "Default")
      (node (ref "U3") (pin "52") (pinfunction "P0.09") (pintype "bidirectional+no_connect")))
    (net (code "50") (name "unconnected-(U3-P0.10-Pad54)") (class "Default")
      (node (ref "U3") (pin "54") (pinfunction "P0.10") (pintype "bidirectional+no_connect")))
    (net (code "51") (name "unconnected-(U3-P0.13-Pad37)") (class "Default")
      (node (ref "U3") (pin "37") (pinfunction "P0.13") (pintype "bidirectional+no_connect")))
    (net (code "52") (name "unconnected-(U3-P0.15-Pad39)") (class "Default")
      (node (ref "U3") (pin "39") (pinfunction "P0.15") (pintype "bidirectional+no_connect")))
    (net (code "53") (name "unconnected-(U3-P0.16-Pad38)") (class "Default")
      (node (ref "U3") (pin "38") (pinfunction "P0.16") (pintype "bidirectional+no_connect")))
    (net (code "54") (name "unconnected-(U3-P0.17-Pad41)") (class "Default")
      (node (ref "U3") (pin "41") (pinfunction "P0.17") (pintype "bidirectional+no_connect")))
    (net (code "55") (name "unconnected-(U3-P0.19-Pad42)") (class "Default")
      (node (ref "U3") (pin "42") (pinfunction "P0.19") (pintype "bidirectional+no_connect")))
    (net (code "56") (name "unconnected-(U3-P0.21-Pad43)") (class "Default")
      (node (ref "U3") (pin "43") (pinfunction "P0.21") (pintype "bidirectional+no_connect")))
    (net (code "57") (name "unconnected-(U3-P0.22-Pad46)") (class "Default")
      (node (ref "U3") (pin "46") (pinfunction "P0.22") (pintype "bidirectional+no_connect")))
    (net (code "58") (name "unconnected-(U3-P0.23-Pad45)") (class "Default")
      (node (ref "U3") (pin "45") (pinfunction "P0.23") (pintype "bidirectional+no_connect")))
    (net (code "59") (name "unconnected-(U3-P0.24-Pad48)") (class "Default")
      (node (ref "U3") (pin "48") (pinfunction "P0.24") (pintype "bidirectional+no_connect")))
    (net (code "60") (name "unconnected-(U3-P0.25-Pad49)") (class "Default")
      (node (ref "U3") (pin "49") (pinfunction "P0.25") (pintype "bidirectional+no_connect")))
    (net (code "61") (name "unconnected-(U3-P0.26-Pad19)") (class "Default")
      (node (ref "U3") (pin "19") (pinfunction "P0.26") (pintype "bidirectional+no_connect")))
    (net (code "62") (name "unconnected-(U3-P0.28-Pad13)") (class "Default")
      (node (ref "U3") (pin "13") (pinfunction "P0.28") (pintype "bidirectional+no_connect")))
    (net (code "63") (name "unconnected-(U3-P0.29-Pad10)") (class "Default")
      (node (ref "U3") (pin "10") (pinfunction "P0.29") (pintype "bidirectional+no_connect")))
    (net (code "64") (name "unconnected-(U3-P0.30-Pad14)") (class "Default")
      (node (ref "U3") (pin "14") (pinfunction "P0.30") (pintype "bidirectional+no_connect")))
    (net (code "65") (name "unconnected-(U3-P0.31-Pad12)") (class "Default")
      (node (ref "U3") (pin "12") (pinfunction "P0.31") (pintype "bidirectional+no_connect")))
    (net (code "66") (name "unconnected-(U3-P1.00-Pad47)") (class "Default")
      (node (ref "U3") (pin "47") (pinfunction "P1.00") (pintype "bidirectional+no_connect")))
    (net (code "67") (name "unconnected-(U3-P1.01-Pad61)") (class "Default")
      (node (ref "U3") (pin "61") (pinfunction "P1.01") (pintype "bidirectional+no_connect")))
    (net (code "68") (name "unconnected-(U3-P1.03-Pad60)") (class "Default")
      (node (ref "U3") (pin "60") (pinfunction "P1.03") (pintype "bidirectional+no_connect")))
    (net (code "69") (name "unconnected-(U3-P1.04-Pad56)") (class "Default")
      (node (ref "U3") (pin "56") (pinfunction "P1.04") (pintype "bidirectional+no_connect")))
    (net (code "70") (name "unconnected-(U3-P1.05-Pad59)") (class "Default")
      (node (ref "U3") (pin "59") (pinfunction "P1.05") (pintype "bidirectional+no_connect")))
    (net (code "71") (name "unconnected-(U3-P1.06-Pad57)") (class "Default")
      (node (ref "U3") (pin "57") (pinfunction "P1.06") (pintype "bidirectional+no_connect")))
    (net (code "72") (name "unconnected-(U3-P1.07-Pad58)") (class "Default")
      (node (ref "U3") (pin "58") (pinfunction "P1.07") (pintype "bidirectional+no_connect")))
    (net (code "73") (name "unconnected-(U3-P1.08-Pad25)") (class "Default")
      (node (ref "U3") (pin "25") (pinfunction "P1.08") (pintype "bidirectional+no_connect")))
    (net (code "74") (name "unconnected-(U3-P1.09-Pad26)") (class "Default")
      (node (ref "U3") (pin "26") (pinfunction "P1.09") (pintype "bidirectional+no_connect")))
    (net (code "75") (name "unconnected-(U3-P1.10-Pad3)") (class "Default")
      (node (ref "U3") (pin "3") (pinfunction "P1.10") (pintype "bidirectional+no_connect")))
    (net (code "76") (name "unconnected-(U3-P1.12-Pad5)") (class "Default")
      (node (ref "U3") (pin "5") (pinfunction "P1.12") (pintype "bidirectional+no_connect")))
    (net (code "77") (name "unconnected-(U3-P1.13-Pad6)") (class "Default")
      (node (ref "U3") (pin "6") (pinfunction "P1.13") (pintype "bidirectional+no_connect")))
    (net (code "78") (name "unconnected-(U3-P1.14-Pad7)") (class "Default")
      (node (ref "U3") (pin "7") (pinfunction "P1.14") (pintype "bidirectional+no_connect")))
    (net (code "79") (name "unconnected-(U3-P1.15-Pad8)") (class "Default")
      (node (ref "U3") (pin "8") (pinfunction "P1.15") (pintype "bidirectional+no_connect")))
    (net (code "80") (name "unconnected-(U3-VBUS-Pad32)") (class "Default")
      (node (ref "U3") (pin "32") (pinfunction "VBUS") (pintype "power_in+no_connect")))))