(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "TLV61070ADBV" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TLV61070ADBV" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (at 1.27 -3.81 0)
      (effects (font (size 1.27 1.27) italic) (justify left) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv61070a.pdf" (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Step-Up DC-DC Converter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2.5-A Boost Converter with 0.5-V Ultra-low Input Voltage, SOT23-6" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TLV61070ADBV_0_1"
      (rectangle (start -5.08 6.35) (end 5.08 -2.54)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "TLV61070ADBV_1_1"
      (pin power_in line (at 7.62 5.08 180) (length 2.54)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -5.08 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 7.62 0 180) (length 2.54)
        (name "FB" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 2.54 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 5.08 0) (length 2.54)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TLV61220DBV" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -5.08 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TLV61220DBV" (at 0 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-6" (at 1.27 -3.81 0)
      (effects (font (size 1.27 1.27) italic) (justify left) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlv61220.pdf" (at 0 2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Step-Up DC-DC Converter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "28-V Output Voltage Boost Converter with Power Diode and Isolation Switch, SOT-23-6" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "SOT?23*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TLV61220DBV_0_1"
      (rectangle (start -5.08 6.35) (end 5.08 -2.54)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "TLV61220DBV_1_1"
      (pin power_in line (at 7.62 5.08 180) (length 2.54)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -5.08 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 7.62 0 180) (length 2.54)
        (name "FB" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 7.62 2.54 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 5.08 0) (length 2.54)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
