(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "TPS7A20_SOT-23" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 2.54 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "TPS7A20_SOT-23" (at 0 0 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/gpn/tps7a20" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "ki_keywords" "TPS7A20" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "300-mA ultra-low-noise low-IQ low-dropout (LDO) linear regulator with high PSRR" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DBV0005A-IPC_A DBV0005A-IPC_B DBV0005A-IPC_C DBV0005A-MFG" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS7A20_SOT-23_0_1"
      (polyline
        (pts
          (xy 5.08 -12.7)
          (xy 25.4 -12.7)
        )
        (stroke (width 0.2032) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 5.08)
          (xy 5.08 -12.7)
        )
        (stroke (width 0.2032) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 25.4 -12.7)
          (xy 25.4 5.08)
        )
        (stroke (width 0.2032) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 25.4 5.08)
          (xy 5.08 5.08)
        )
        (stroke (width 0.2032) (type default))
        (fill (type none))
      )
      (pin power_in line (at 0 0 0) (length 5.08)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 30.48 -10.16 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -5.08 0) (length 5.08)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 0 -10.16 0) (length 5.08)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 30.48 0 180) (length 5.08)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS7A2033PDVBR" (extends "TPS7A20_SOT-23")
    (property "Reference" "U" (at 0 2.54 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "TPS7A20_SOT-23" (at 0 0 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "ki_keywords" "TPS7A20" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "300-mA ultra-low-noise low-IQ low-dropout (LDO) linear regulator with high PSRR" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DBV0005A-IPC_A DBV0005A-IPC_B DBV0005A-IPC_C DBV0005A-MFG" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
  (symbol "TPS7A20_X2SON" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 2.54 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "TPS7A20_SOT-23" (at 0 0 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "Package_SON:Texas_X2SON-4_1x1mm_P0.65mm" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/gpn/tps7a20" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "ki_keywords" "TPS7A20" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "300-mA ultra-low-noise low-IQ low-dropout (LDO) linear regulator with high PSRR" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DBV0005A-IPC_A DBV0005A-IPC_B DBV0005A-IPC_C DBV0005A-MFG" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS7A20_X2SON_0_1"
      (polyline
        (pts
          (xy 5.08 -12.7)
          (xy 25.4 -12.7)
        )
        (stroke (width 0.2032) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 5.08 5.08)
          (xy 5.08 -12.7)
        )
        (stroke (width 0.2032) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 25.4 -12.7)
          (xy 25.4 5.08)
        )
        (stroke (width 0.2032) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 25.4 5.08)
          (xy 5.08 5.08)
        )
        (stroke (width 0.2032) (type default))
        (fill (type none))
      )
      (pin input line (at 0 -5.08 0) (length 5.08)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "TPS7A20_X2SON_1_1"
      (pin unspecified line (at 30.48 0 180) (length 5.08)
        (name "OUT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 30.48 -10.16 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 0 0) (length 5.08)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 0 -10.16 0) (length 5.08)
        (name "THRM" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TPS7A2033PDQNR" (extends "TPS7A20_X2SON")
    (property "Reference" "U" (at 0 2.54 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "TPS7A20_SOT-23" (at 0 0 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "ki_keywords" "TPS7A20" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "300-mA ultra-low-noise low-IQ low-dropout (LDO) linear regulator with high PSRR" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DBV0005A-IPC_A DBV0005A-IPC_B DBV0005A-IPC_C DBV0005A-MFG" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
  )
)
